Topologies

Select a host from the left frame to display the corresponding topology. A TOPO name (as created in the Topology Maintenance -> Merge Topologies section) can also be selected. Use the [Search] field to search by topology name or host name, partial names can be used. Hosts are grouped 'Hosts 1' to 'Hosts N' when there is too many slaves to display them all at the same time. Select 'Hosts N' to see more details. The Island List functions will automatically break the 'MASTER' topo into smaller topos. Devices that have no fibre channel links in common (directly or indirectly) are in separate islands.