## Storage Automated Diagnostic Environment
Diagnostic Guide

6120ondg | 6120ondg - tests the Fibre Channel loops inside and outside the Sun StorEdge 6120 array.
6120test | 6120test - tests the functionality of the Sun StorEdge 6120 array LUNs
6120volverify | volverify - Runs manual parity checks on Sun StorEdge T3, T3+, and 6120 array volumes
a3500fctest | a3500fctest - verifies functionality of Sun StorEdge A3500FC disk tray
a5ksestest | a5ksestest - tests Sun StorEdge A5000 and A5200 arrays
a5ktest | a5ktest - tests the functionality of disks in the Sun StorEdge A5000 and A5200 array
brocadetest | brocadetest - diagnose Brocade Silkworm Fibre Channel switches
checkcron | checkcron - check crontab entries
clearcache | clearcache -clears Storage Automated Diagnostic Environment cache files
config_solution | config_solution - creates a configuration snapshot during the manufacturing and upgrading of Sun StorEdge 3900 and 6900 series and Sun StorEdge 6320 and 6320SL system solu- tions.
d2disktest | d2disktest - tests the functionality of the Internal Sun StorEdge D2 Array disk
daksestest | daksestest - tests Sun Fire V880 FC-AL disk backplanes
daktest | daktest - tests the Sun Fire V880 FC-AL disk
dex | dex - Device Exerciser for Sun StorEdge arrays
discman | discman - discovery manager
disk_inquiry | disk_inquiry - disk-only version of the inquiry program
disktest | disktest - tests the functionality of fibre channel disks
echotest3510 | echotest3510 - initiates an echo test between two devices on a fabric
fcdisktest | fcdisktest - tests the functionality of internal fibre chan- nel disk
fctapetest | fctapetest - tests the functionality of Fibre Channel tape drives
ifptest | ifptest - tests functionality of the PCI FC-100 Fibre Channel-Arbitrated loops (FC-AL) card
jnitest | jnitest - tests the functions of the Sun StorEdge 2 Gbyte PCI Fibre Channel Network Adapter JNI boards.
lbf | lbf - A loop back frame diagnostic utility program that tests Fibre Channel-Arbitrated loops (FC-AL)
linktest | linktest - diagnose Sun StorEdge network passive Fibre Chan- nel components
loopmap3510 | loopmap3510 - Fibre channel loop position map for a 3510 fibre channel
looptest3510 | looptest3510 - initiates an internal or external loopback test
ondg | ondg - tests the Fibre Channel loops inside and outside the Sun StorEdge array.
qlctest | qlctest - tests the functions of the Sun StorEdge 1 Gbyte and 2 Gbyte PCI and cPCI Fibre Channel Network Adapter boards.
ras_admin | ras_admin - command line interface to Storage Automated Diagnostic Environment
ras_discover | ras_discover - discovers devices and updates the configura- tion file on the slave and the master.
ras_install | ras_install - executes the ras_install command to start the Storage Automated Diagnostic Environment services.
ras_patchlist | ras_patchlist - executes PatchPro software and creates a list of devices and required patches.
ras_remote | ras_remote - executes Storage Automated Diagnostic Environ- ment commands remotely.
ras_revcheck | ras_revcheck - checks the software, hardware, and firmware revision levels.
ras_upgrade | ras_upgrade - upgrades a set of devices using PatchPro.
rasagent | rasagent - monitors, collects, and reports information about Sun storage products.
sanbox | sanbox - access the SANbox switch diagnostic facilities
save_password | save_password - change the Storage Automated Diagnostic Environment admin password
se2_configcheck | se2_configcheck - Verify the configuration of a Sun StorEdge Solution System
se_configcheck | se_configcheck - Verify the configuration of a Sun StorEdge Solution System
showBypassDevice3510 | showBypassDevice3510 - displays the bypass status of all devices on a specified loop
snapshot | snapshot - take snapshot of configuration
socaltest | socaltest - tests the SOC+ host adapter card
stresstest | stresstest - Checks for possible SAN errors.
switch2test | switch2test - diagnose Sun StorEdge Network FC switch-8 and switch-16 2 Gbyte Fibre Channel switches
switchtest | switchtest - diagnose Sun StorEdge Network Fibre Channel switch-8 and switch-16 switches
t3command | t3command - run predefined array commands
t3test | t3test - tests the functionality of the Sun StorEdge T3 and T3+ array LUNs
t3volverify | volverify - Runs manual parity checks on Sun StorEdge T3, T3+, and 6120 array volumes
test3510 | test3510 - read/write buffer test for the 3510
testt3 | testt3 - retrieve tokens from a Sun StorEdge T3 array
vediag | vediag - Runs virtualization engine diagnostics through SLICD
veluntest | veluntest - tests the functionality of the virtualization engine by accessing the VLUNs.
volverify | volverify - Runs manual parity checks on Sun StorEdge T3, T3+, and 6120 array volumes