## CLI Man Pages

The man pages describe the features of the Storage Automated Diagnostic Environment 2.3. Man pages can be invoked from the command line interface (CLI) and will be updated for the Storage Automated Diagnostic Environment 2.3 in `troff` format.

Each task will not have a man page. The following man pages are available:

Test | Description
--- | ---
`6120ofdg.1m` | Tests the functionality of the Sun StorEdge 6020 array.
`6020volverify.1m` | Runs manual parity checks on Sun StorEdge 6020 array volumes.
`6120ondg.1m` | Tests the Fibre Channel loops inside and outside the Sun StorEdge 6020 array.
`a3500fctest.1m` | Verifies functionality of Sun StorEdge A3500FC disk tray.
`a5ksestest.1m` | Tests Sun StorEdge A5000 and A5200 arrays.
`a5ktest.1m` | Tests the functionality of disks in the Sun StorEdge A5000 and A5200 array.
`brocadetest.1m` | Diagnose Brocade Silkworm Fibre Channel switches.
`checkcron.1m` | Check `crontab` entries.
`clearcache.1m` | Clears Storage Automated Diagnostic Environment cache files.
`config_solution.1m` | Creates a configuration snapshot during the manufacturing and upgrading of Sun StorEdge 6920 system solutions.
`d2disktest.1m` | Tests the functionality of the Internal Sun StorEdge D2 Array disk.
`daksestest.1m` | Tests Sun Fire V880 FC-AL disk backplanes.
`daktest.1m` | Tests the Sun Fire V880 FC-AL disk.
`dex.1m` | Device Exerciser for Sun StorEdge arrays.
`discman.1m` | Discovery manager.
`disk_inquiry.1m` | Disk-only version of the inquiry program.
`disktest.1m` | Tests the functionality of fibre channel disks.
`fcdisktest.1m` | Tests the functionality of internal fibre channel disks.
`fctapetest.1m` | Tests the functionality of Fibre Channel tape drives.
`ifptest.1m` | Tests functionality of the PCI FC-100 Fibre Channel-Arbitrated loops (FC-AL) card.
`linktest.1m` | Diagnose Sun StorEdge network passive Fibre Channel components.
`qlctest.1m` | Tests the functions of the Sun StorEdge 1 Gbyte and 2 Gbyte PCI and cPCI Fibre Channel Network Adapter boards.
`ras_admin.1m` | Command line interface to Storage Automated Diagnostic Environment.
`ras_discover.1m` | Discovers devices and updates the configuration file on the slave and the master.
`ras_install.1m` | Executes the `ras_install` command to start the Storage Automated Diagnostic Environment services.
`ras_patchlist.1m` | Executes PatchPro software and creates a list of devices and required patches.
`ras_remote.1m` | Executes Storage Automated Diagnostic Environment commands remotely.
`ras_revcheck.1m` | Checks the software, hardware, and firmware revision levels.
`ras_upgrade.1m` | Upgrades a set of devices using PatchPro.
`rasagent.1m` | Monitors, collects, and reports information about Sun storage products.
`sanbox.1m` | Access the SANbox switch diagnostic facilities.
`save_password.1m` | Change the Storage Automated Diagnostic Environment admin password.
`se_configcheck.1m` | Verify the configuration of a Sun StorEdge Solution System (3900/6900).
`se2_configcheck.1m` | Verify the configuration of a Sun StorEdge Solution System (6320/6920).
`snapshot.1m` | Take a snapshot of configuration.
`socaltest.1m` | Tests the SOC+ host adapter card.
`stresstest.1m` | Checks for possible SAN errors.
`switch2test.1m` | Diagnose Sun StorEdge Network FC switch-8 and switch-16 2 Gbyte Fibre Channel switches.
`switchtest.1m` | Diagnose Sun StorEdge Network Fibre Channel switch-8 and switch-16 switches.
`t3ofdg` | Tests the functionality of the Sun StorEdge T3 array.
`t3test` | Tests the functionality of the Sun StorEdge T3 and T3+ array LUNs.
`t3volverify` | Runs manual parity checks on Sun StorEdge T3 array volumes.
`testt3` | Runs manual parity checks on Sun StorEdge T3 array volumes.
`vediag` | Runs virtualization engine diagnostics through SLICD.
`veluntest` | Tests the functionality of the virtualization engine by accessing the VLUNs.
`volverify` | Runs manual parity checks on Sun StorEdge T3, T3+, and 6020 array volumes.