## Event Summary Page

Field | Description
Event Type | Displays the name of the event; for example,`t3.AlarmEvent`.
Severity | Displays the severity icon: Blue - Minor Yellow - Major Red - Critical Black - Down
Component | Displays the FRU-level component about which the event was generated.
Action Required | Displays a Y (action required) or N (no action required-information only). If the event is actionable, the event grid will also display probable cause and recommended action.
EventNo. | Displays the event number, used for tracking purposes.
Description | Displays the date and the time the event occurred.
Information | Displays background information that is relevant to this specific event.
Probable Cause | Explains why the event probably occurred. This information will only appear if the event is actionable.
Recommended Action | Displays suggested steps for problem resolution. This information will only appear if the event is actionable.

##

## Monitoring Devices Using Device Report

For each component, the user has the ability to expand the device and gather information down to each FRU. For this example, the Sun StorEdge 6120 array and its components are shown, though similar detailed information is available for each device that the host monitors.