## Creating a Topology Snapshot

Use the Topology Snapshot function to create and update the topology view from the host or to review error details.

Before you create a Topology snapshot, make sure there are no failed over paths. If there are failed over paths, the Topology view does not properly display them.

1. From the Topology Maintenance window, click the Topology Snapshot link.

The Topology Snapshot window is displayed.

2. Select the check box that corresponds to the topology and click Create Selected Topologies. If you want to create a snapshot of all topologies, click Create All Topologies.

Note -

If one or more Brocade switches are included in the system topology, you must supply the Brocade-defined password for the Brocade switch in order to display zone information for the switch.

While the system creates the selected topology, the status is in one of two states:

- Running-Discovery is running on the selected host, and the system creates and retrieves the selected topology.
- Done-The topology has been created and is ready for you to retrieve.
- Click the Review link to review the error details, if applicable.
- Click the Clear link in the Delete column to clear a selected topology.

The Last Snapshot column contains the date of the last time a topology was extracted from this host.

The Last Master column contains the date the last Master Topology was sent back to that host.