AP In             (PCT)

DESCRIPTION
"AP In" represents the number of inbound asynchronous processing (AP) 
requests for a given "Transid" received from remote CICS regions.


VALUES
The value of "AP In" is a number.


INTERPRETATION
There are two different ways that a remote CICS region can initiate an AP
request into the local system. First, the remote application program can issue 
a START command with a Transid that is defined as remote in the remote CICS
region's Program Control Table (PCT). Second, the remote application can specify
the SYSID as a parameter to the START command, in which case there is no need
to look up the Transid's entry in the PCT.


CONCLUSIONS
This datapoint gives you the ability to see the number of inbound AP requests 
for a specific Transid. 
