LU Name           (TCT)

DESCRIPTION
"LU Name" displays the logical unit name of all 3270 entries in the TCT Screen,
as well as for active Transaction Route (TR) entries. 


VALUES
The "LU Name" field displays an alphanumeric string that is always 8 characters 
or less.


INTERPRETATION
Sun MTPScan populates this field for all 3270 entries, active or not. This includes
terminals preconfigured in the 3270 Devices portion of the Sun MTP Terminal
Control Table (TCT). For preconfigured terminals, "LU Name" shows the value (of
the same name) as set in the Sun MTP TCT. The TCT Screen also shows the "LU Name"
for active TR surrogate entries since the underlying representation is 
essentially a 3270-type connection.


CONCLUSIONS
A preconfigured TR entry in the 3270 Devices portion of the Sun MTP TCT also sets
the LU Name field. However, Sun MTPScan only displays the "LU Name" for active TR
entries since the actual value gets set upon connection. In other words, Sun MTP
ignores the LU Name field for preconfigured TR entries, and learns of the actual
"LU Name" on the fly.
