Session           (TCT)

DESCRIPTION
Sun MTPScan displays a "Session" value for '3270', 'EPI', and 'TR' entries. The
"Session" is a number that identifies a particular connection between a device
and some portion of the region or communication software on a machine that
allows the device to communicate with a Sun MTP system.


VALUES
"Session" takes a nonzero integer value if a "Session" exists. Otherwise, this
datapoint does not display anything.


INTERPRETATION
The interpretation of "Session" depends on the "Type" of entry. The following
kinds of entries may display a "Session" value:

3270 - the XPUx Server dynamically assigns the "Session" id for the connection
       between itself and the terminal device

EPI  - the value is used internally by Sun MTP to identify the connection

TR   - identifies the "Session" number between the transaction program and the 
       PU2.1 Server, dynamically assigned by the PU2.1 Server


CONCLUSIONS
Use the value to identify diagnostic entries in the trace files for a particular
session. 
