Device Name       (TCT)

DESCRIPTION
"Device Name" displays a form of device identifier based on the "Type" of entry.
This field typically shows a terminal's definition as known to the client term-
inal handler process to help find the exact location of the terminal.


VALUES
The value of "Device Name" is dependent on the "Type" of entry. The following
chart shows what kind of value to expect for a given "Type":

EPI    - an EPI-specific terminal identifier, at most 8 characters

Local  - On a UNIX platform, this is the full pathname of a physical device for 
         a tty connection used by unikixl to identify the tty; usually of the 
         form /dev/tty* with at most 20 characters displayed

Remote - same as Local, but on the remote system 

TN3270 - TN3270-specific identifier, usually containing the "Pid", at most 9
         characters, used by unikixtn

TR     - the 12 character terminal name as known to the remote region, a 
         concatenation of the Applid and the remote Termid


INTERPRETATION
The "Device Name" helps identify the origin of a TCT Screen entry. Sun MTPScan sets
this field for all types of entries except for 3270 and Free entries.


CONCLUSIONS
