901 San Antonio Road Palo Alto, CA 94303-4900 USA 650 960-1300 Fax 650 969-9131

SunVideo^™ Plus 1.3 Installation

Part No. 804-6949-10 October 1999, Revision A

Sun Microsystems, Inc.

Send comments about this document to: docfeedback@sun.com

Copyright 1999Sun Microsystems, Inc. All rights reserved.

This product or document is protected by copyright and distributed under licenses restricting its use, copying, distribution, and decompilation. No part of this product or document may be reproduced in any form by any means without prior written authorization of Sun and its licensors, if any.Third-party softwar e, including font technology ,is copyrighted and licensed from Sun suppliers.

Parts of the product may be derived from Berkeley BSDsystems, licensed from the University of California. UNIX is a register ed trademark in the U.S. and other countries, exclusively licensed through X/Open Company ,Ltd.

Sun, Sun Microsystems, the Sun logo, AnswerBook, SunVideo, and Solaris are trademarks, register ed trademarks, or service marks of Sun Microsystems, Inc. in the U.S. and other countries. All SPARC trademarks are used under license and are trademarks or register ed trademarks of SPARC International, Inc. in the U.S. and other countries. Products bearing SPARC trademarks are based upon an architectur e developed by Sun Microsystems, Inc.

The OPEN LOOK and Sun™ Graphical User Interface was developed by Sun Microsystems, Inc. for its users and licensees. Sun acknowledges the pioneering efforts of Xerox in resear ching and developing the concept of visual or graphical user interfaces for the computer industry .Sun holds a non-exclusive license from Xerox to the Xerox Graphical User Interface, which license also covers Sun’slicensees who implement OPEN LOOK GUIs and otherwise comply with Sun’swritten license agreements.

RESTRICTED RIGHTS :Use, duplication, or disclosur e by the U.S. Government is subject to restrictions of FAR 52.227-14(g)(2)(6/87) and FAR 52.227-19(6/87), or DFAR 252.227-7015(b)(6/95) and DFAR 227.7202-3(a). DOCUMENT ATION IS PROVIDED “AS IS” AND ALL EXPRESS OR IMPLIED CONDITIONS, REPRESENTATIONS AND W ARRANTIES, INCLUDING ANY IMPLIED W ARRANTY OF MER- CHANT ABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NON-INFRINGEMENT , ARE DISCLAIMED, EXCEPT T O THE EXTENT THA T SUCH DISCLAIMERS ARE HELD T O BE LEGALLY INVALID

3

Copyright 1999Sun Microsystems, Inc. Tous droits réservés.

Ce produit ou document est protégé par un copyright et distribué avec des licences qui en restreignent l’utilisation, la copie, la distribution, et la décompilation. Aucune partie de ce produit ou document ne peut être reproduite sous aucune forme, par quelque moyen que ce soit, sans l’autorisation préalable et écrite de Sun et de ses bailleurs de licence, s’ily en a. Le logiciel détenu par des tiers, et qui compr end la technologie relative aux polices de caractèr es, est protégé par un copyright et licencié par des fournisseurs de Sun.

Des parties de ce produit pourr ont être dérivées des systèmes Berkeley BSDlicenciés par l’Université de Californie. UNIX est une mar que déposée aux Etats-Unis et dans d’autres pays et licenciée exclusivement par X/Open Company , Ltd.

Sun, Sun Microsystems, le logo Sun, AnswerBook, SunVideo, et Solaris sont des mar ques de fabrique ou des mar ques déposées, ou mar ques de service, de Sun Microsystems, Inc. aux Etats-Unis et dans d’autres pays. Toutes les mar ques SPARC sont utilisées sous licence et sont des mar ques de fabrique ou des mar ques déposées de SPARC International, Inc. aux Etats-Unis et dans d’autres pays. Les produits portant les mar ques SPARC sont basés sur une architectur e développée par Sun Microsystems, Inc.

L’interface d’utilisation graphique OPEN LOOK et Sun™ a étédéveloppée par Sun Microsystems, Inc. pour ses utilisateurs et licenciés. Sun reconnaît les efforts de pionniers de Xerox pour la recherche et le développement du concept des interfaces d’utilisation visuelle ou graphique pour l’industrie de l’informatique. Sun détient une licence non exclusive de Xerox sur l’interface d’utilisation graphique Xerox, cette licence couvrant également les licenciés de Sun qui mettent en place l’interface d’utilisation graphique OPEN LOOK et qui en outr e se conforment aux licences écrites de Sun.

CETTE PUBLICATION ESTFOURNIE "EN L’ETAT"ETAUCUNE GARANTIE, EXPRESSEOU IMPLICITE, N’ESTACCORDEE, YCOMPRIS DES GARANTIES CONCERNANT LA VALEUR MARCHANDE, L’APTITUDEDE LA PUBLICATION A REPONDRE A UNE UTILISATION PARTICULIERE, OU LEFAIT QU’ELLENE SOIT PAS CONTREFAISANTE DE PRODUIT DE TIERS.CE DENI DE GARANTIE NE S’APPLIQUERAIT PAS, DANS LA MESURE OU ILSERAIT TENU JURIDIQUEMENT NUL ETNON AVENU.

4

SunVideo Plus 1.3Installation

This document describes how to install the SunVideo ™ Plus hardwar e and softwar e. The SunVideo Plus 1.3 Installation Guide, provided with this installation kit, is a multilingual document of the instr uctions described here.

Installation Kit

The SunVideo Plus 1.3 Installation Kit includes:

SunVideo Plus 1.3 card SunVideo Plus 1.3 softwar e (CD) Antistatic wriststrap SunVideo Plus 1.3 Installation Guide

System Requirements

You can install SunVideo Plus softwar e on any SPARC™ system running Solaris™ 2.5.1, Solaris 2.6, or Solaris 7 operating envir onments. 1

Installing the SunV ideo Plus Card

1. Install the SunV ideo Plus card according to the installation procedures for PCI-bus cards provided with your Sun ™ system.

2. After installing the SunV ideo Plus card and securing your system enclosure, boot your system by typing:

hostname# reboot -- -r

2 6

SunV ideo Plus 1.3 Software Contents

Contents Description Solaris Software Suppor t

Docs/
 C/
 de/
 es/
 fr/
 it/
 ja/
 ko/
 sv/
 zh/
 zh_TW.BIG5

Translated User ’sGuide English German Spanish French Italian Japanese Korean Swedish Simplified Chinese Traditional Chinese (BIG5)

Common to each Solaris release

Common/
 Packages/
 SUNWo1kpdu
 SUNWopi
 SUNWopi1k
 SUNWsvpab
 SUNWvtsvp

Runtime libraries OPI device support OPI-1x00 runtime libraries AnswerBook ™ SunVTS™ test

All packages under the

Common/ directory

support the Solaris 2.5.1, Solaris 2.6, and Solaris 7 operating envir onments.

3

Once installed, the SunVideo Plus 1.3 softwar e resides in

/etc/opt/SUNWo1kp, /opt/SUNWo1kp, and /opt/SUNWopi. The

XIL Runtime pipeline softwar e resides in /usr/openwin.

Removing Previous Software Releases

You must remove any previous releases of the SunVideo Plus softwar e before installing any new softwar e packages.

1. Log in as superuser .

2. Uninstall previous SunV ideo Plus software packages.

Solaris_2.5.1/
 Packages/
 SUNWo1kpd.u
 SUNWo1kpx

Device driver XIL1.2 Runtime

Solaris 2.5.1 Har dwar e: 4/97, 8/97, and 11/97 operating envir onment

Solaris_2.6/
 Packages/
 SUNWo1kpd.u
 SUNWo1kpx

Device driver XIL1.3 Runtime

Solaris 2.6 and Har dwar e: 3/98 and 5/98 operating envir onment

Solaris_7/
 Packages/
 SUNWo1kpd.u
 SUNWo1kpx

Device driver XIL1.3 Runtime

Solaris 7 and Har dwar e: 3/99, 5/99, 8/99, 11/99 operating envir onment

Contents Description Solaris Software Suppor t

4 8

Note – SUNWo1kpu and SUNWo1kpd are core packages; hence, be sure that these packages are removed last by the pkgrm command (as shown below).

Remove SunVideo Plus 1.0 by typing:

Remove SunVideo Plus 1.1 or 1.2 by typing:

Installing the SunV ideo Plus 1.3 Software

The SunVideo Plus 1.3 softwar e is provided on the CD included with your SunVideo Plus installation kit.

1. Log in as superuser (root).

2. Insert the SunV ideo Plus 1.3 CD into the CD-ROM drive connected to your system.

hostname# /usr/sbin/pkgrm SUNWvtsvp SUNWsvpab SUNWo1kpu
SUNWo1kpd

hostname# /usr/sbin/pkgrm SUNWvtsvp SUNWsvpab SUNWo1kpx
SUNWo1kpu SUNWo1kpd

5

If your system is running Volume Manager , it should automatically mount the CD-ROM to the

/cdrom/sunvideo_plus_1_3 directory.

If your system is not running Volume Manager , mount the CD-ROM as follows:

3. Install the SunV ideo Plus 1.3 software using the pkgadd command:

a. Install the base software packages for the Solaris 2.5.1, Solaris 2.6, and Solaris 7 operating environments:

Choose all to install the base packages.

b. Proceed to install specif ic Solaris release software packages.

hostname# mkdir -p /cdrom/sunvideo_plus_1_3
hostname# mount -F hsfs -r /dev/dsk/c0t6d0s2
/cdrom/sunvideo_plus_1_3

hostname# cd /cdrom/sunvideo_plus_1_3/Common/Packages
hostname# /usr/sbin/pkgadd -d .

6 10

To install the Solaris 2.5.1 Har dwar e: 4/97, 8/97, and 11/97 operating envir onment, type:

Choose all.

To install the Solaris 2.6 operating envir onment, type:

Choose all.

To install the Solaris 7 operating envir onment, type:

Choose all.

hostname# cd /cdrom/sunvideo_plus_1_3/Solaris_2.5.1/
Packages
hostname# /usr/sbin/pkgadd -d .

hostname# cd /cdrom/sunvideo_plus_1_3/Solaris_2.6/
Packages
hostname# /usr/sbin/pkgadd -d .

hostname# cd /cdrom/sunvideo_plus_1_3/Solaris_7/
Packages
hostname# /usr/sbin/pkgadd -d .

7

4. After the software has been installed, unmount and eject the CD-ROM:

5. Reboot your workstation:

This enables the operating system to recognize the SunVideo Plus card.

Accessing User Documentation

To access the SunVideo Plus 1.3 User’s Guide, including translated versions:

Go to http://www.sun.com/desktop/products/Graphics/

SunVideoPlus_Download.html and download the appropriate

document.

hostname# cd /
hostname# umount /cdrom/sunvideo_plus_1_3
hostname# eject cdrom

hostname# reboot -- -r

8