APIs in Category: snmp | API version 1.12

snmp-community-add snmp-community-delete snmp-community-delete-all snmp-disable snmp-enable snmp-get snmp-get-next snmp-status snmp-trap-delete snmp-trap-disable snmp-trap-enable snmp-trap-list snmp-trap-load snmp-trap-reset snmp-trap-set snmp-traphost-add snmp-traphost-delete

NetApp Manage ONTAP

snmp-community-add | [top]

> Adds a community to the list of communities.

> Input Name | Range | Type | Description
> access-control |  | string | Access control for the community. Possible values are "ro" (read-only) and "rw" (read-write). But, only "ro" (read-only) communities are supported.
> community |  | string | Community name to be added.

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-community-delete | [top]

> Deletes a community from the list of communities.

> Input Name | Range | Type | Description
> access-control |  | string | Access control for the community. Possible values are "ro" (read-only) and "rw" (read-write). But, only "ro" (read-only) communities are supported.
> community |  | string | Community name to be deleted.

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-community-delete-all | [top]

> Deletes all the communities.

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-disable | [top]

> Disables snmp protocol.

snmp-enable | [top]

> Enables snmp protocol.

snmp-get | [top]

> Retrieves the value of a snmp object.

> Input Name | Range | Type | Description
> object-id |  | string | Fully qualified object identifier of a snmp object. Only numeric OID's (ex: .1.3.6.1.4.1.789.1.1.1.0) are allowed.
> Output Name | Range | Type | Description
> is-value-hexadecimal |  | boolean optional | If true, the string returned in 'value' is the hexadecimal representation of the octet string returned by a snmp call to the object-id. This output is not present if 'value' is a normal string.
> value |  | string | Value of the snmp object specified through the input argument "object-id".

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-get-next | [top]

> This is used to retrieve the next OID in the mib tree of data. Instead of returning the data you requested, it returns the next OID in the tree and its value. Unlike the snmp-get api, this api does return data for a OID which is too short or is missing the index part of the OID.

> Input Name | Range | Type | Description
> object-id |  | string | Object Identifier of a snmp object. The OID can be a fully qualified OID or a partial OID. Only numeric OID's (ex: .1.3.6.1.4.1.789.1.1.1.0) are allowed.
> Output Name | Range | Type | Description
> is-value-hexadecimal |  | boolean optional | If true, the string returned in 'value' is the hexadecimal representation of the octet string returned by a snmp call to the object-id. This output is not present if 'value' is a normal string.
> next-object-id |  | string | Object Identifier of the next snmp object in the mib.
> value |  | string | Value of the snmp object reported through the output argument "next-object-id".

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-status | [top]

> Returns configuration information of the SNMP agent daemon.

> Output Name | Range | Type | Description
> communities |  | community-info[] | Returns a list of communities and their access control settings.
> contact |  | string | Contact name.
> is-trap-enabled |  | boolean | Retuns "true" if traps are enabled. "false" otherwise.
> location |  | string | Location name.
> traphosts |  | traphost-info[] | Returns a list of registered trap hosts followed by their IP addresses. Only resolvable trap hosts are returned. If a host name cannot be found in /etc/hosts for a previously registered IP address, its name defaults to a string representation of its IP address.

snmp-trap-delete | [top]

> Delete a user defined trap.

> Input Name | Range | Type | Description
> trap-name |  | string | Name of the trap to be deleted.

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-trap-disable | [top]

> Disables snmp traps.

snmp-trap-enable | [top]

> Enables snmp traps.

snmp-trap-list | [top]

> List all user defined traps and their attributes.

> Output Name | Range | Type | Description
> trap-list |  | trap-info[] | The list of user defined snmp traps and their attributes.

> Errno | Description
> EONTAPI_EINVAL |  |
> EONTAPI_ENOMEM |  |

snmp-trap-load | [top]

> Loads traps from a specified file.

> Input Name | Range | Type | Description
> filename |  | string | Name, including full PATH, of the file specifying the user defined traps. Example: /etc/MyTraps.txt would open the MyTraps.txt file located on the filer's /etc directory.

> Errno | Description
> EONTAPI_EINVAL |  |
> EONTAPI_ENOENT |  |
> EONTAPI_ENOMEM |  |

snmp-trap-reset | [top]

> Reloads one or all user defined traps from registry.

> Input Name | Range | Type | Description
> trap-name |  | string optional | Name of the trap to be reset. If absent, all traps are reset.

snmp-trap-set | [top]

> Set the named user defined trap and the enumerated attribute(s). The trap-name must be specified for this api.

> Input Name | Range | Type | Description
> trap-def |  | trap-info | Characterizes a user defined trap and its attributes.

> Errno | Description
> EONTAPI_EINVAL |  |
> EONTAPI_ENOENT |  |
> EONTAPI_ENOMEM |  |

snmp-traphost-add | [top]

> Adds a host to the list of trap hosts.

> Input Name | Range | Type | Description
> host |  | string | Specify the host to be added. Host may be specified in Domain Name format such as MyHost.MyNetwork.com, or as an IP address such as 10.20.30.40. If a Domain Name is used, the host must resolve to an IP address.

> Errno | Description
> EONTAPI_EINVAL |  |

snmp-traphost-delete | [top]

> Deletes a host from the list of trap hosts.

> Input Name | Range | Type | Description
> host |  | string | Specify the host to be added. Host may be specified in Domain Name format such as MyHost.MyNetwork.com, or as an IP address such as 10.20.30.40. If a Domain Name is used, the host must resolve to an IP address.

> Errno | Description
> EONTAPI_EINVAL |  |

Element definition: community-info | [top]

> Information about a single community.

> Name | Range | Type | Description
> access-control |  | string | Access control of the community. Possible values are "ro" (read-only), and "rw" (read-write).
> community |  | string | Community name.

Element definition: trap-info | [top]

> Information about a single user defined trap.

> Name | Range | Type | Description
> OID |  | string optional | Specifies the OID of the MIB object that is queried to determine the trap's value. This attribute is set to "undefined" on output if not explicitly specified in trap definition. If absent on input, there is no default value, and trap definition is incomplete.
> active |  | string optional | Notification state of trap. Possible values are "on" indicating agent will deliver notification if triggered, "off" indicating trap is inactive, and "incomplete" indicating one or more of the required attributes have not been defined. The default value for a fully defined trap is "off".
> backoff-calculator |  | string optional | Specifies a method by which the frequency of trap evaluation may be modified. Possible values are "step-backoff", "exponential-backoff", and "no-backoff" This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is "no-backoff".
> backoff-multiplier |  | integer optional | Factor by which interval is multiplied when exponential-backoff method used. Used with "exponential-backoff" calculator. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is 1. Range may be [0..2^31-1].
> backoff-step |  | integer optional | Time in seconds by which evaluation interval is increased when step-backoff method used. Used with "step-backoff" calculator. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is 0. Range may be [0..2^31-1].
> current-value |  | integer optional | Value of trap at time of query. On input, this attribute is ignored. Range may be [-2^31..2^31-1].
> edge-1 |  | integer optional | Threshold value at which trap is triggered. If not specified on input, the default value is 2^31-1. Range may be [-2^31..2^31-1].
> edge-1-direction |  | string optional | Sets the direction of travel across the edge-1 threshold beyond which the trap is triggered. Possible values are "up", and "down". If not specified on input, the default value is "up".
> edge-2 |  | integer optional | Threshold value at which trap is triggered. Used with double-edge-trigger condition. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is 0. Range may be [-2^31..2^31-1].
> edge-2-direction |  | string optional | Sets the direction of travel across the edge-2 threshold beyond which the trap is triggered. Possible values are "up", and "down". Used with double-edge-trigger condition. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is "down".
> interval |  | integer optional | Time in seconds between evaluations of the trap. A trap can send data only as often as it is evaluated. If not specified on input, the default value is 3600 seconds (1-hour). Range may be [0..31536000].
> interval-offset |  | integer optional | Time in seconds until the first trap evaluation. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is 0. Range may be [0..31536000].
> message |  | string optional | Message associated with trap. May be either a literal string, or specifies an OID. This attribute is set to "undefined" on output if not explicitly specified in trap definition. If absent on input, there is no default value, and trap definition is incomplete.
> priority |  | string optional | Priority level of trap. Possible values (in descending order of severity) are "emergency", "alert", "critical", "error", "warning", "notification", "informational", or "debug". This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is "notification".
> rate-interval |  | integer optional | Time in seconds over which rate of change is calculated from sample data. This attribute may be absent on output if not explicitly specified in trap definition. If absent on input, the default is 0. Range may be [0..2^31-1].
> trap-name |  | string | Name of the trap given by the user. Note that trap-name may not contain embedded periods.
> trigger |  | string optional | Sets the condition under which the trap will send a notification. Possible values are "single-edge-trigger", "double-edge-trigger", or "level-trigger". This attribute is set to "undefined" on output if not explicitly specified in trap definition. If absent on input, there is no default value, and trap definition is incomplete.

Element definition: traphost-info | [top]

> Information about a single registered trap host.

> Name | Range | Type | Description
> host-name |  | string | Name of the trap host given by the user. Can be one of the following: hostname, ip-address, or alias Hostname will be a fully qualified Domain Name.
> ip-address |  | string | IP address of the trap host.