# Configuring Multiple Systems for Scripting

User Access: Administrators

There are two ways to configure multiple Service Processors for scripting:

- Execute the procedure to configure the client machine on which you will be running scripts for each Service Processor.
- Set up the trust relationship or add your public key file on an initial machine and use the autoconfiguration feature to duplicate the configuration on each of the additional machines. See the server documentation for details about how to perform autoconfiguration.

Sample Scripts

Several example shell scripts are available in your Network Share Volume (NSV) directory titled scripts/samples. Use these examples as a starting point when you develop your own scripts.

See the sensor get and inventory get hardware commands for information about how to retrieve the product ID, board revision, and PRS revision.

Related Topics

Configuring Shell Scripts

Configuring the Client for Scripting