# SP Miscellaneous Subcommands

The following subcommands manage miscellaneous Service Processor functions:

Subcommand | Description
--- | ---
sp create test events | Tests and validates different types of configurations you may be considering for the Service Processor.
sp get port 80 | Retrieves the last port 80 postcode from the PRS Port80 register.
sp get status | Returns the status of the overall system.
sp get tdulog | Captures data and stores it on the Service Processor in compressed format.
sp autoconfigure | Configures a Service Processor with the same configuration as that of another Service Processor.
sp reset | Restores selected settings of the Service Processor to the default factory configuration.
sp reboot | Restarts the Service Processor.

Related Topics

System Management Commands

SP Command