# IPMI Reset Subcommand

access: Managers

Resets IPMI information back to default factory settings.

> ipmi reset {-s | –sdrr} {-c | –config} {-p | –password} {-a | –all}

Argument | Description
--- | ---
{-s | –sdrr} | Copies the original database file to pstore.
{-c | –config} | Deletes the configuration file and global enables.
{-p | –password} | Deletes the password file.
{-a | –all} | Performs the functions of all the parameters.

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_NoPermission | 6 | Not authorized to perform this operation.

Related Topics

System Management Commands

IPMI Command