# IPMI Disable PEF Subcommands

access: Managers

This command disables the PEF feature of IPMI. It simplifies this process because it allows you to disable any manufacturer-installed event filters without the the need a series of IPMI commands against each filter.

> ipmi disable pef

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_NoPermission | 6 | Not authorized to perform this operation.

Related Topics

System Management Commands

IPMI Command