# SP Update Flash Subcommands

The following subcommands manage the Service Processor flash:

Subcommand | Description
--- | ---
sp update flash all | Sets the update flag to start the full flash update on the next Service Processor reset.
sp update flash applications | Copies the Value-Add file to the Value-Add component of the Service Processor flash.
sp update diags | Updates the diagnostics to a newer version.

Related Topics

System Management Commands

SP Command