# SP Get SNMP Destinations Subcommand

access: All users

Displays the available SNMP destinations (IP address or hostname) to which the Service Processor is configured to send. Many networking programs use this information to identify the machine.

> sp get snmp-destinations

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_RPCTimeout | 2 | Request was issued, but was not serviced by the server. RPC procedure timed out and the request may or may not have been serviced by the server.
NWSE_RPCConnRefused | 3 | RPC connection refused.
NWSE_NoMemory | 8 | Insufficient memory.
NWSE_UnknownError | 15 | Miscellaneous error not captured by other errors.
NWSE_FileError | 18 | File open, missing, or read or write error occurred.

Related Topics

System Management Commands

SP Command