# SP Add Logical-Group Member Subcommand

access: manager

Adds a new Service Processor IP address or platform hostname to an already-defined logical group.
These logical groups can be used to initiate operations on a set of remote Service Processors from a master Service Processor.

> > sp add logical-group member {–g | --group} GROUP_NAME
> > {{–m | --member} [SP_IP_HOSTNAME | {-p | --platform} PLATFORM_HOSTNAME | UUID]

> Argument | Description
> --- | ---
> {–g | --group} | The name of an existing logical group.
> {–m | --member} | The Service Processor IP address or Service Processor hostname .
> {-p | --platform} | The platform hostname.

Return Codes

Following are the return values for this command:

Code | Numeric Code | Code | Description
--- | --- | --- | ---
NWSE_Success | 0 | NWSE_Success | Command successfully completed.
NWSE_InvalidUsage | 1 | NWSE_InvalidUsage | Invalid usage: bad parameter usage, conflicting options specified. The remote mount point was not specified.
NWSE_InvalidArgument | 4 | NWSE_InvalidArgument | One or more arguments were incorrect or invalid. The local directory does not exist.
NWSE_NoPermission | 6 | NWSE_NoPermission | Not authorized to perform this operation.

Related Topics

System Management Commands

SP Command