# System Management Commands

The Service Processor includes a suite of commands that enables management and monitoring of the system. These commands are called the Systems Management Commands. From the command line, for example, you can write data-driven scripts that automate configuration of multiple machines.

The SM Commands take arguments, perform one or more actions, and display the result or text to the standard output device. Commands are grouped by similar function. Most command groups have several subcommands that support functions in that group.

Command | Description
--- | ---
access | Allows the authorized user to manage and monitor access control and security features of the Service Processor.
diags | Manages diagnostics tests included with your system.
inventory | Allows the authorized user to monitor system hardware and software inventory.
ipmi | Allows the authorized user to manage IPMI functions.
platform | Allows the authorized user to manage and monitor platform activities.
sensor | Reports or sets the value of an environmental sensor or control.
sp | Allows the authorized user to manage and monitor Service Processor configurations.

Notes

- Every command returns a return code when it completes.

Related Topics

Return Codes

Scripting Guidelines

Glossary