OBSOLETE Patch-ID# 107716-26
Keywords: security gfxp raptor driver pgxconfig man ddx
Synopsis: Obsoleted by: 107716-27 SunOS 5.7: PGX32 Graphics Patch
Date: Oct/28/2003


Install Requirements: Additional instructions may be listed below                      
                      Reboot after installation                      
                      
Solaris Release: 7

SunOS Release: 5.7

Unbundled Product: 

Unbundled Release: 

Xref: 

Topic: 

Relevant Architectures: sparc.sun4u

BugId's fixed with this patch: 4225083 4228453 4230383 4230823 4231943 4236513 4237268 4238896 4241319 4247777 4274934 4276955 4298419 4313132 4329407 4340678 4344436 4347028 4352469 4357957 4372518 4373617 4377807 4383508 4396037 4398941 4417836 4417842 4417849 4420220 4431012 4467936 4470386 4500303 4500323 4502647 4502887 4506566 4517899 4522502 4633850 4715825 4728662 4740340 4776309 4800057 4802284 4863629 4897594 4897600 4898192

Changes incorporated in this version: 4897594 4897600 4802284 4898192 4863629

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

	/platform/sun4u/kernel/drv/sparcv9/gfxp
	/platform/sun4u/kernel/drv/sparcv9/raptor
	/usr/openwin/server/etc/pgxresinfo
	/usr/sbin/pgxconfig
	/usr/share/man/man1m/pgxconfig.1m
    /platform/sun4u/kernel/drv/raptor
    /usr/openwin/bin/gfxres
    /usr/openwin/server/modules/ddxTSIgfx.so.1
/platform/sun4u/kernel/drv/gfxp

Problem Description:

4897594 PGX-32 DDX should not call system()
4897600 PGX-32 DDX buffer overflow
4802284 Xinerama system with PGX32 cards hangs with s9 patch.
4898192 TSI ddx has faults
4863629 pgx32: interactive configuration should not show "16 only".
 
(from 107716-25)
4715825 Xsun server grows huge and hangs display(monitors)
 
(from 107716-24)
4776309 cursor too big when pgx32 installed
 
(from 107716-23)
4800057 Patch 109154-16 lost the fix for bug 4728662 of rev -15
 
(from 107716-22)
4740340 Icons and scrollbars are distorted in Citrix in 16 or 256 color mode.
 
(from 107716-21)
4728662 displaying some URL with PGX32 causes Xserver to crash
 
(from 107716-20)
Revision produced to address patch packaging issues.
 
(from 107716-19)
4633850 Iconifying windows under CDE corrupts the backdrops
 
(from 107716-18)
4502887 PGX32: 108652-37 causes the monitor power-saving starts instead of screen blank
 
(from 107716-17)
4517899 black painted selection screens in webstart install on machines with GFX cards
4506566 Problem w/ Animator demo on PGX32  (pixmaps problem)
4522502 pgx32 24+8 mode: XShmPutImage has problems with pixels with MSB set
 
(from 107716-16)
4500323 *gfxres* suffers from a buffer overflow
4500303 *pgxconfig* contains buffer overflow
4502647 add hook to disable long PIO
 
(from 107716-15)
4431012 cannot adjust "1280x1024x85 -24only true -depth 24" with latest patches
4467936 memory leak in gfxpAttach()
4470386 pgxconfig should be setuid
4420220 SwingSet2 garbages the screen and crashes the X server on pgx32 board
 
(from 107716-14)
4417836 cannot run pgx32 rev 06 in 1280x1024x85 and 8+24 bit depth with latest patches
4417842 noise with patch # 107851-12 on 21" monitor w/ resolution 1280x1024x85
4417849 depth is reported inconsistently w/ latest patch # 107851-12 at 1280x1024x85
 
(from 107716-13)
4373617 dual headed syntax in Xserver file does not work on raptor systems
4352469 Performance degradation using PGX32 cards with Ultra-60 in xinerama mode
4396037 VSW502 XGetImage-2 kill Xsun on 2 pgx32s 1280x1024 with xinerama top-bottom
 
(from 107716-12)
4377807 PGX32: performance issue.
4398941 pgxconfig does not work with TFT Monitor PN 365-1394
 
(from 107716-11)
4383508 PGX32: can't set colormap correctly on Solaris 2.6
4372518 pgxconfig has security problem
 
(from 107716-10)
4357957 Sunvts soft memory read errors were observed during the -05 qualification
 
(from 107716-09)
4340678 PGXconfig -res \? display wrong informations with Monitor 365-1383
4344436  pixel noise on screen during colormap updates - pgx32
4347028 PGX32: GFXconfig does not show that 1152x900 is supported resolution.
 
(from 107716-08)
4329407 Xsun process eats up a large percentage of the CPU cycles
 
(from 107716-07)
4313132 PGX32 displays large bitmaps/pixmaps incorrectly
 
(from 107716-06)
4298419 GFXconfig: Bus error when see help by 'H' on interactive mode.
 
(from 107716-05)
4276955 Drag and drop splits cursor on dual or triple headed pgx32 systems
4274934 SunVTS 3.3 fails with memory errors when Mango is installed as Console
 
(from 107716-04)
4230383 E3500 causes a FATAL RESET while running the vsw5 graphics testsuite
 
(from 107716-03)
4241319 PGX32 doesn't draw part of  lines and circles when zoomed the data.
4247777 Cannot do a gui install on a machine with a mango card
 
(from 107716-02)
4238896 man page incomplete/incorrect
4228453 pgx32 paniced on resume on gfxpPMResume+0x4a4: call bcopy
4231943 PGX32 caused system hang with execute init0 from Openwindows on UE450
4237268 pgx32 is power managed when screen-saver is turned off on CDE's Stylemanager
4236513 systems with mango card as console frequently freeze or hang on restore
4230823 System gets crashing with any shutdown commands on Pgx32 card
 
(from 107716-01)
4225083 pgx32 refuses to suspend if system is left idle for 30 minutes

Patch Installation Instructions:
--------------------------------
For Solaris 2.0 - 2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7 - 9 releases, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd 104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
After installing this patch, reboot the system to load the newly
installed driver.

README -- Last modified date:  Thursday, January 20, 2005

