##

### To Power Down All Arrays (Partial Shutdown)

Note - These partial shutdown steps apply to the Sun StorEdge 6300 storage system. The Partial Shutdown button is enabled only if you or Sun Service personnel have installed a USB cable between the remote power relay and the Storage Service Processor. If you perform a partial shutdown on arrays in the Sun StorEdge 6300 system, a Restart button is available from the General link at the Administration Page the next time you display this page.

1. Click General at the Administration tab.
2. Click the Partial Shutdown button.

When you click the Partial Shutdown button, the Storage Service Processor and accessory tray remain powered on and accessible. The arrays are powered down.

### To Restart All Arrays (from Partial Shutdown)

Note - You can restart arrays in the Sun StorEdge 6300 storage system if you or Sun Service personnel have installed a USB cable between the remote power relay and the Storage Service Processor and you have performed a partial shutdown. If you perform a partial shutdown on arrays in the Sun StorEdge 6300 system, a Restart button is available from the General link at the Administration tab the next time you display this page.

1. Click General at the Administration tab.
2. Click the Restart button to reset and power on the arrays.