##

### To Change Network Settings (Sun StorEdge 6100)

1. Click Array and Action Selection at the Administration tab.
2. Check the box next to the array that you want to configure, and click Network Settings.
3. Click RARP if you want your array to obtain an IP address from a RARP server on the same subnet.

Caution - You must use a known IP address when you register the array with the managment software. If the IP address changes, the managment software will be unable to manage the array due to an unknown IP address.

4. Click Fixed to manually configure network settings.
5. To manually configure the network settings, type the following entries:

IP Address: type the Storage Service Processor or array IP address

Gateway IP: type the gateway IP address

Netmask: type the subnet mask IP address

6. Click Save to save the new settings.