##

### Power Management (Sun StorEdge 6100)

The General link on the Administration tab to enable the admin user to power down the system or the array. The individual array power down is useful when adding trays or other components to an array.

### To Power Down the Array

1. Click the Array and Action Selection at the Administration tab.
2. Select one (6100 only) array in the table under the Array Power Management section.

Note - The Array Name link in the table, when clicked, enables you to view array details and change tray settings as described in Array Details and Tray Reconfiguration.

3. Click the Shutdown button.

To power on the array, you must manually power it on.

4. Confirm the power down action.

This button powers off the selected array. Repeat these steps to power down more than one array.

### To Restart the Array

1. Click the Array and Action Selection at the Administration tab.
2. Select an array.
3. Click the Restart button to reset and power on the selected array.

Repeat these steps to restart more than one array.