# Array Configuration and Management

Caution - Do not configure the Sun StorEdge 6000 Family arrays by using the array Telnet interface and this web browser user interface at the same time. Use the Telnet interface or web browser user interface.
Do not use more than one instance of the software at a time to access or configure the same storage arrays or systems. For example, two storage users using the software from two different machines cannot add the same volumes to a volume group each user is creating or modifying.

The Array Selection main menu is the default page that is displayed after you log into the software. The Array Selection in on the right-hand pane, and a Tree menu is located in the left-hand pane.

This page enables you to check detailed system and device health status by launching the Storage Automated Diagnostic Environment application. (This application is installed by default on the Sun StorEdge 6300 Storage Service Processor. It must be installed on the local Solaris host for the Sun StorEdge 6100 arrays to be able to launch it from this page.)

See also Array Details and Tray Reconfiguration.

From this page you can configure and manage your array. See the following sections:

- Viewing the Graphic Array Overview
- Managing Storage Pools
- Array Registration (Sun StorEdge 6100)
- Array Configuration
- Duplicating Array Settings
- Managing Profiles
- Managing Volumes
- Managing Volume Groups
- Managing Initiators
- Managing Initiator Groups
- Viewing the Access Matrix