##

## Array Root Password (Sun StorEdge 6100)

Sun StorEdge 6120 arrays are shipped from the factory with no password set for the array's root user. Logging into the web browser with a blank password will grant you access to manage arrays.

### To Assign a Root Password for an Array

1. Telnet to the Sun StorEdge 6120 array using the array's IP address.

       % telnet array_IP_address

       Trying array_IP_address ...

       Connected to array_IP_address

       Escape character is '^]'.

       Unauthorized access is prohibited.

2. Log in as root. Do not type a password.

       Login: root

       Password:

       6120 Release 3.0.3 Mon Mar 10 15:47:42 PST 2003 (10.4.36.137)

       Copyright (C) 1997-2003 Sun Microsystems, Inc.

       All Rights Reserved.

3. Issue the passwd command. Do not type a password for the OLD password.

       prompt> passwd

       OLD password:

       NEW password: new_password

       NEW password (confirm): new_password

       prompt>

4. Log out of the telnet session.