##

### Network Settings

Note - See also Firewall Port Filtering (Sun StorEdge 6300).

The Network page displays the current network IP address and other settings for the system. Typically, these values are set at the factory or by Sun service engineers or authorized service personnel.

Caution - Changing these settings might disable access temporarily, and require the user to re-log in. If invalid network settings are supplied, it may disable access to the application.

### To Change Network Settings (Sun StorEdge 6300)

1. Click Network at the Administration tab.
2. Click DHCP if your system obtains its network settings from a Dynamic Host Configuration Protocol (DHCP) server.

This choice is the default setting for the system.

3. Click Fixed to manually configure network settings.
4. To manually configure the network settings, type the following entries:

IP Address: type the Storage Service Processor or array IP address

Gateway IP: type the gateway IP address

Netmask: type the subnet mask IP address

Name Server: type the domain name server (DNS) IP address.

Domain Name: type the domain name, if required for Sendmail to function properly in your network.

5. Click Save to save the new settings.