sun.com | docs.sun.com |  | How To Buy | My Sun | Worldwide Sites |

A B C D E F G H I J K L M N O P Q R S T U V W X Y Z

File Formats | install-server.conf(4)

- NAME
- SYNOPSIS
- DESCRIPTION
- PARAMETERS
- EXAMPLE
- ATTRIBUTES
- SEE ALSO

## NAME

> install-server.conf - SMCT configuration file to configure the network for the installation server

## SYNOPSIS

> `SMCT_DEFAULT_CONFIG_DIR/models/install-server.conf`
> `config-dir/models/install-server.conf`

## DESCRIPTION

> Do not use the SMCT tool with the current patch level of the Foundation Services product.

> The `install-server.conf` configuration file enables network configuration between the prototype machine and the installation server. The prototype machine and the installation server must be on the same subnet.

## PARAMETERS

> The following are the parameters in the `install-server.conf` file:

> >     # install-server network configuration file
> >     name install-server-name
> >     ip install-server-IP
> >     netmask netmask
> >     nic nic-name
> >     router y/n

> - install-server-name

>   Host name of the installation server.

> - install-server-IP

>   IP address of the installation server.

> - netmask

>   Netmask of the private network between the installation server and the prototype machine.

> - nic-name

>   Interface name of the installation server's private network.

> - y/n

>   By default, SMCT verifies that the installation server does not act as a router, that is, the file `/etc/notrouter` exists. This avoids the broadcasting of routing information from the private network over the public network. To enable routing, set the parameter to `y`. The default value is `n`.

> The `name`, `ip`, `netmask`, and `nic` parameters are mandatory and must be configured. The `router` parameter is optional.

## EXAMPLE

> The following is an example of an `install-server.conf` file:

> >     # install-server network configuration file
> >     name installserv1
> >     ip 10.100.1.1
> >     netmask 255.255.255.0
> >     nic hme1
> >     router n

## ATTRIBUTES

> See `attributes`(5) for descriptions of the following attributes:

> ATTRIBUTE TYPE | ATTRIBUTE VALUE
> --- | ---
> Architecture | SPARC
> Availability | SUNWnhsmc
> Interface Stability | Evolving

## SEE ALSO

> `flcreate`(1M), `fldeploy`(1M), `flinstall`(1M), `master-system.conf`(4)

Netra HAS FS 2.1 | Go To Top | Last Changed September 2004

Company Info | Contact | Copyright 2004 Sun Microsystems, Inc. All rights reserved. Use is subject to license terms.