sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Index Next
## Receiving Notifications With the NMA The NMA can be used to "listen" for notifications of the following cluster events: A node joins or leaves the cluster A master node or vice-master node is elected The maximum number of times that the Daemon Monitor attempts to restart a daemon or group of daemons is reached The maximum number of times that the Daemon Monitor attempts to restart a daemon or group of daemons is changed by the NMA The current number of times that the Daemon Monitor has attempted to restart a daemon or group of daemons is reset to zero by the NMA A nametag is created by the Daemon Monitor A nametag is removed by the Daemon Monitor For more information, see the Netra High Availability Suite Foundation Services 2.1 6/03 NMA Programming Guide.
Previous Contents Index Next

Copyright 1994-2004 Sun Microsystems