sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Next
Chapter 8 # I in node A peer node that is using the Foundation Services and can communicate with other peer nodes. An "in node" can be a master-eligible node, a diskless node, or a dataless node. The master node and vice-master node must always be "in nodes". See also out node. installation server Installation hardware required by the `nhinstall` tool, and to install manually. An installation server installs the software load onto the cluster by using the Solaris JumpStart™ software. The installation server can be a portable machine. IP (Internet Protocol) IP mirroring See replication. IPMP (IP multipathing) A system that enables a server to have multiple network ports connected to the same subnet.
Previous Contents Next

Copyright 1994-2004 Sun Microsystems