Patch-ID# 113388-02
Keywords: security RSC bugs
Synopsis: RSC 2.2.1 patch
Date: Oct/29/2002

Install Requirements: None                      
                      
Solaris Release: 9

SunOS Release: 5.9

Unbundled Product: Remote System Control

Unbundled Release: 2.2.1

Xref: 

Topic: RSC 2.2.1 patch

Relevant Architectures: sparc

BugId's fixed with this patch: 4368760 4520586 4521771 4528896 4531159 4532903 4613870 4625032 4660874 4670940 4674391 4674561 4713019 4726272 4726292

Changes incorporated in this version: 4368760 4520586 4521771 4528896 4531159 4532903 4613870 4625032 4660874 4674391 4674561 4713019 4726272 4726292

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/rsc/doc/en/html/alert_sc.htm
/opt/rsc/doc/en/html/copyrigh.htm
/opt/rsc/doc/en/html/event_co.htm
/opt/rsc/doc/en/html/modem_ap.htm
/opt/rsc/doc/en/html/rsc_pref.htm
/opt/rsc/doc/en/html/rscix.htm
/opt/rsc/doc/en/html/rsctoc.htm
/opt/rsc/doc/en/html/title.htm
/opt/rsc/doc/en/html/ucm_adm_.htm
/opt/rsc/doc/en/html/ucm_conf.htm
/opt/rsc/doc/en/html/ucm_gui_.htm
/opt/rsc/doc/en/html/ucm_hwin.htm
/opt/rsc/doc/en/html/ucm_obp_.htm
/opt/rsc/doc/en/html/ucm_over.htm
/opt/rsc/doc/en/html/ucm_shel.htm
/opt/rsc/doc/en/html/ucm_trou.htm
/opt/rsc/doc/en/html/ups_app.htm
/opt/rsc/doc/en/pdf/user_guide.pdf
/opt/rsc/lib/java/com/sun/rsc/internal/l10n/RscData.class
/opt/rsc/lib/java/com/sun/rsc/internal/ssp/RSCEvents.class
/opt/rsc/lib/locale/en/html/logs.html
/usr/platform/SUNW,Sun-Fire-280R/lib/images/rscfw
/usr/platform/SUNW,Sun-Fire-280R/rsc/rsc-config
/usr/platform/SUNW,Sun-Fire-280R/rsc/rscadm
/usr/platform/SUNW,Ultra-250/lib/images/rscfw

Problem Description:

4368760 Invalid message displayed when Littleneck rsc-config is run in error on Javelin
4520586 rscadm error message for non-RSC systems is incorrect
4521771 console buffer(s) must be able to capture error reset output from obp
4528896 Power supply numbering is incorrect on littleneck
4531159 SFV480 CPU1 and CPU2 fans are numbered incorrectly by RSC
4532903 XIR event log item is logged as a standard RSC initiated host reset w/o an alert
4613870 RSC serial port hangs within 15 minutes if idle when not using ethernet port
4625032 Internal ethernet loopback selftest fails if ip_mode=none
4660874 gui help section "About Logs Files" needs some changes to reflect updated UG.
4674391 rsc uses malformed mail from: addresses
4674561 rcsadm date -s sets incorect seconds
4713019 /opt/rsc/bin /opt/rsc/lib are duplicate file pathnames in multiple packages
4726272 Modem read implementation is incorrect and does not obey timeout
4726292 RSC does not properly handle non-strict TAP protocol
 
(from 113388-01)
 
4670940 Are rsc cards snmp capabilities affected by CA-2002-03?

Patch Installation Instructions:
-------------------------------- 
 
1. Become super-user.
 
2. Use the 'patchadd' utility included with Solaris 9 for installing
   this patch.  For example:
 
	% /usr/sbin/patchadd /var/spool/patch/113388-01
 
   Reference the man page for patchadd(1M) for more information on
   'patchadd'.
 
3. Use 'patchrm' to remove the patch if necessary.

Special Install Instructions:
----------------------------- 
 
The user must run the rscadm command when patch installation has
completed in order to download the RSC firmware to the RSC
hardware. Use this command line:
 
/usr/platform/<platform-name>/rsc/rscadm download
       /usr/platform/<platform-name>/lib/images/rscfw
 
where <platform-name> is obtained from uname -i,
e.g. SUNW,Sun-Fire-280R.

README -- Last modified date:  Tuesday, October 29, 2002

