Patch-ID# 117255-01
Keywords: rsc patch bugs
Synopsis: RSC 2.2.2 S8 bug fixes
Date: Sep/22/2004


Install Requirements: None                      
                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: Remote System Control

Unbundled Release: 2.2.2

Xref: 

Topic: 

Relevant Architectures: sparc
NOTE: sun4u

BugId's fixed with this patch: 4754151 4833403 4888644 4900490 4910618 4913407 4921990 4924826 4924838 4925290 4925291 4926655 4926666 4927532 4927567 4928246 4928266 4928986 4935143 4939696 4944222 4949479 4959724 4959729 4967244 4974474 4987954 4989514 4989696 4991471 4993067 4995318 4997456 5007843 5008596 5008653 5010381 5018952 5020379

Changes incorporated in this version: 4754151 4833403 4888644 4900490 4910618 
4913407 4921990 4924826 4924838 
4925290 4925291 4926655 4926666 
4927532 4927567 4928246 4928266 
4928986 4935143 4939696 4944222 
4949479 4959724 4959729 4967244 
4974474 4987954 4989514 4989696 
4991471 4993067 4995318 4997456 
5007843 5008596 5008653 5010381 
5018952 5020379

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/rsc/doc/en/html/alert_sc.htm
/opt/rsc/doc/en/html/copyrigh.htm
/opt/rsc/doc/en/html/event_co.htm
/opt/rsc/doc/en/html/figures/e250_log.jpg
/opt/rsc/doc/en/html/index.html
/opt/rsc/doc/en/html/modem_ap.htm
/opt/rsc/doc/en/html/rsc_pref.htm
/opt/rsc/doc/en/html/rscix.htm
/opt/rsc/doc/en/html/rsctoc.htm
/opt/rsc/doc/en/html/shared/contents.gif
/opt/rsc/doc/en/html/shared/home.gif
/opt/rsc/doc/en/html/shared/index.gif
/opt/rsc/doc/en/html/shared/next.gif
/opt/rsc/doc/en/html/shared/previous.gif
/opt/rsc/doc/en/html/title.htm
/opt/rsc/doc/en/html/ucm_adm_.htm
/opt/rsc/doc/en/html/ucm_conf.htm
/opt/rsc/doc/en/html/ucm_gui_.htm
/opt/rsc/doc/en/html/ucm_hwin.htm
/opt/rsc/doc/en/html/ucm_obp_.htm
/opt/rsc/doc/en/html/ucm_over.htm
/opt/rsc/doc/en/html/ucm_shel.htm
/opt/rsc/doc/en/html/ucm_trou.htm
/opt/rsc/doc/en/html/ups_app.htm
/opt/rsc/doc/en/pdf/user_guide.pdf
/opt/rsc/lib/images/about_banner.gif
/opt/rsc/lib/java/com/sun/rsc/internal/pages/AlertFrame.class
/opt/rsc/lib/java/com/sun/rsc/internal/pages/AlertInfo.class
/opt/rsc/lib/java/com/sun/rsc/internal/pages/PagingDialog.class
/opt/rsc/lib/java/com/sun/rsc/internal/ssp/BasePlatformSupport.class
/opt/rsc/lib/java/com/sun/rsc/internal/util/version.properties
/opt/rsc/lib/locale/en/html/alerts.html
/opt/rsc/lib/locale/en/html/comm.html
/opt/rsc/lib/locale/en/html/logs.html
/opt/rsc/lib/locale/en/html/toggle_LED.html
/opt/rsc/lib/platform-files/Sun-Fire-480R/cs-base.gif
/opt/rsc/lib/platform-files/Sun-Fire-480R/platform.properties
/opt/rsc/lib/platform-files/Sun-Fire-880/dak-base.gif
/opt/rsc/lib/platform-files/Sun-Fire-880/platform.properties
/opt/rsc/lib/platform-files/Sun-Fire-V490/supportedfeatures.txt
/opt/rsc/lib/platform-files/Sun-Fire-V890/supportedfeatures.txt
/usr/platform/SUNW,Sun-Fire-280R/lib/images/rscfw
/usr/platform/SUNW,Sun-Fire-280R/lib/librsc.so.2
/usr/platform/SUNW,Sun-Fire-280R/rsc/rsc-config
/usr/platform/SUNW,Sun-Fire-280R/rsc/rscadm
/usr/platform/SUNW,Ultra-250/lib/images/rscfw

Problem Description:

4754151 RSC intermittently stops responding to ping and telnet
4833403 rsc 1.14 allows multiple instances of a single console window
4888644 Remove RSC debug service on TCP port
4900490 RSC build procedure does not support Solaris 8
4910618 Environmental thresholds are not correct in RSC
4913407 RSC2.2.2b19 ver of GUI logs.html is different that previous ver (orun missing)
4921990 rsc-config fails to execute on V890
4924826 system in standby gives "DisplayTemps: ERROR ---> 3d0004" message in showenviron
4924838 rscadm reset is not working, but rscadm resetrsc -s is
4925290 Battery Backup Status, Modem and pager setup need to be removed from GUI
4925291 rscadm modem_setup option should be removed from on-line help
4926655 TPE Link Test is disabled when the "Enable TPE test" box is checked off.
4926666 setlocator on, then setlocator off from cli but the GUI still shows the led ON
4927532 Cannot download firmware - error: Failed to identify flash ROM!
4927567 envPollNull message in loghistory after every rsc reset
4928246 No "system powered off" alert received, nothing in loghistory
4928266 Versions don't match in "About RSC"
4928986 Need to support new service controller card
4935143 I2C: Cannot Open i2c Device, exiting program message rec'd from environment cmd
4939696 Problems with VXDiag AFT mode tests on new SC hardware
4944222 Restore orun log documentation
4949479 rscadm download gets a bootfail on first try
4959724 RSC must support set/showlocator CLI commands on platform
4959729 RSC GUI must support new system indicator panel layout
4967244 RSC packages for S9U6 need to be in freshbitted format
4974474 RSC must support new flash RAM part
4987954 Incorrect message/ No data received on GUI "show environment" when power off
4989514 GUI help section should remove all content related to pager alerts
4989696 IO Fan Failures are reported incorrectly by RSC on Sebring and V480
4991471 Platforms using RSC card log "Unrecognized SC type" message
4993067 Permissions are wrong on file in SUNWrsc freshbitted package
4995318 There is no mention of the V490 server in the locator section of the GUI Help
4997456 GUI Server Types window is incorrectly labeling V480/V880 servers
5007843 AC Power events are not recognized by RSC on Silverstone
5008596 rsc-config allows modem and pager to be configured
5008653 Temperatures tab is missing in RSC GUI on Sebring only
5010381 Celsius to Fahrenheit toggle no longer works in RSC GUI on Sebring
5018952 unplugged power supply displays temperature failure in gui
5020379 RSC GUI Front Panel images use incorrect product names

Patch Installation Instructions:
-------------------------------- 
 
1. Become super-user.
 
2. Use the 'patchadd' utility included with Solaris 9 for installing RSC patch
   117255-01. For example:
 
	% /usr/sbin/patchadd /var/spool/patch/117255-01
 
  Reference the man page for patchadd(1M) for more informatino on 'patchadd'.
 
3. Use 'patchrm' to remove the patch if necessary.

Special Install Instructions:
----------------------------- 
 
 
The user must run the rscadm command when patch installation has completed in
order to download the RSC firmware to the RSC hardware. Use this command line:
 
/usr/platform/<platform-name>/rsc/rscadm download
       /usr/platform/<platform-name>/lib/images/rscfw
 
where <platform-name> is obtained from uname -i, e.g. SUNW,Sun-Fire-280R.
 
Note: This patch may be applied only to RSC from the Computer Systems
Supplement CD packaged with Solaris 8 02/04 (HW4).

README -- Last modified date:  Wednesday, September 22, 2004

