Patch-ID# 106887-02
Keywords: sunvideo, rtvc, xil
Synopsis: SunOS 5.7:  SunVideo 1.4 Patch
Date: May/04/1999

Solaris Release: 7

SunOS Release: 5.7

Unbundled Product: 

Unbundled Release:

Relevant Architectures: sparc 

BugId's fixed with this patch: 4197200 4233236

Changes incorporated in this version: 4233236

Patches accumulated and obsoleted by this patch:

Patches which conflict with this patch: 

Patches required with this patch:

Obsoleted by: 

Files included with this patch: 
 
/usr/openwin/lib/xil/devhandlers/xilCompress_UYVY.so.2
/usr/openwin/lib/xil/devhandlers/xilCompute_CellBSUNWrtvc.so.2
/usr/openwin/lib/xil/devhandlers/xilCompute_JpegSUNWrtvc.so.2
/usr/openwin/lib/xil/devhandlers/xilCompute_Mpeg1SUNWrtvc.so.2
/usr/openwin/lib/xil/devhandlers/xilCompute_UYVYSUNWrtvc.so.2
/usr/openwin/lib/xil/devhandlers/xilIO_SUNWrtvc.so.2

Problem Description: 

(from 106887-02)
 4233236 Send blank images instead of invalid ones when capture fails with 
         SUNWrtvc-13

(from 106887-01)
 4197200  Image get shrunk when xil_color_convert is called (PAL only)

Patch Installation Instructions: 
-------------------------------- 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch."

For Solaris 7 release, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

        example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

        example# patchrm 104945-02

For additional examples please see the appropriate man pages.


Special Install Instructions: 
----------------------------- 

After installing this patch, reboot the system to load the newly
installed driver.
