Patch-ID# 113218-04
Keywords: DR loops cpu power PCI DMA handle
Synopsis: SunOS 5.9: patch pcipsy
Date: 15/Sep/02

Solaris Release: 9

SunOS release: 5.9

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.9: patch pcipsy

	***********************************************************
	NOTE: This patch may contain one or more OEM-specific platform ports.
	      See the appropriate OEM_NOTES file within the patch for
	      information specific to these platforms.
 
	      DO NOT INSTALL this patch on an OEM system if a corresponding
	      OEM_NOTES file is not present (or is present, but instructs not
	      to install the patch), unless the OEM vendor directs otherwise.
	***********************************************************

BugId's fixed with this patch: 4114317 4640542 4669486 4674788 4678396 4682258 4697219 4704996 

Changes incorporated in this version: 4678396

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 112233-02 (or newer)

Obsoleted by: 

Files included with this patch:

/etc/driver_aliases
/platform/SUNW,Ultra-Enterprise-10000/kernel/drv/pcipsy
/platform/SUNW,Ultra-Enterprise-10000/kernel/drv/sparcv9/pcipsy
/platform/sun4u/kernel/drv/pci_pci
/platform/sun4u/kernel/drv/pcipsy
/platform/sun4u/kernel/drv/sparcv9/pci_pci
/platform/sun4u/kernel/drv/sparcv9/pcipsy
/platform/sun4u/kernel/drv/sparcv9/pcisch

Problem Description:

4678396 PCI DMA handle allocation overhead

(from 113218-03)

4640542 Add XMITS support for SF15K
4697219 prtdiag crashes when a property doesn't exist
4704996 dman driver hardcodes the binding names of on board devices

(from 113218-02)

4669486 CE messaging too verbose and unclear
4674788 Cheetah/Cheetah+ invalid AFSR logging should be more descriptive
4682258 PCI ECC correctable errors can report wrong dimm or whole bank of dimms

(from 113218-01)

4114317 DR operations hang after a few loops when cpu power control is also running

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

NOTE  : To get the complete fix of bug 4114317 (DR operations hang after a few
        loops when cpu power control is also running), please install the 
        following patches:

        113024-01       (or newer)      wrsm
        113219-01       (or newer)      fhc
        113220-01       (or newer)      upa64s 
        112233-01       (or newer)      KU patch



