Patch-ID# 114608-09
Keywords: sun fire 15k hpost axq
Synopsis: SMS 1.3: hpost patch for SMS 1.3
Date: May/14/2004


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.3

Xref: 

Topic: SMS 1.3: hpost patch for SMS 1.3

Relevant Architectures: sparc

BugId's fixed with this patch: 4753686 4803319 4807422 4814913 4815141 4818581 4820554 4822152 4823642 4835023 4839477 4840328 4843254 4844692 4850839 4851622 4863496 4866952 4868483 4868987 4871417 4875660 4878056 4880549 4880811 4890963 4892492 4898641 4905481 4926900 4928390 4935970 4936225 4936971 4943893 4961973 4967964 4969557 4971396 4974501 4975645 4985137 4990454 5023600 5030572 5030612 5030965

Changes incorporated in this version: 4943893 4975645 4990454 5023600 5030572 5030612 5030965

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.3/bin/hpost
/opt/SUNWSMS/SMS1.3/bin/redx
/opt/SUNWSMS/SMS1.3/ict/5015694-12-01.esvf
/opt/SUNWSMS/SMS1.3/lib/libxcpost.so

Problem Description:

4943893 dstop during POST - AXQ and SDI are inconsistant
4975645 Allow MaxCPU in split expander with AXQ 6.3
4990454 FAIL CDC DIMM when running warm reboot test w/ AXQ6.3
5023600 wfail should recognize EXBs reset during operation
5030572 Skip hsPCI+ workaround for AXQ 6.3
5030612 force_axq_xmits_throttle_vector doesn't work if only slot 0 present.
5030965 Accept AXQ 6.3 without warning
 
(from 114608-08)
 
4936225 known bad processor did not get indicted by post as expected
4961973 Illegal GDTransid device code in split expander configuration
4967964 Post needs to support and run lbist for axq 6.3
4969557 Bad server_retval during download should call out a fru
4971396 POST gives wrong message with MCPU DR in split slot configuration
4974501 POST support for AXQ 6.3 with split expanders
4985137 hpost -Q missing AXQ workaround for hPCI+.
 
(from 114608-07)
 
4926900 post needs to accept PCI IOC 2.5 on wPCI cards without warning
4928390 Not all Slot 0 errors masked on AXQ deconfigure
4935970 Desire per-bus .postrc control of PCI mode for pre-GA hardware.
4936971 Automate AXQ workaround for hsPCI+
 
(from 114608-06)
 
4892492 hpost during -Q does not reset empty or missing io slots on hsPCI+ boards
4898641 Frequency measurement should retry on any incorrect value.
4905481 asic_config_axq() failing EXB with AXQ failure
 
(from 114608-05)
 
4850839 Processor failed inappropriately after memory FAIL
4866952 post hangs when SB proc times out on Host Test 201; locks up SC
4868483 Don't use unreliable DX errors for diagnosis
4868987 hpost points to CSB0 as the primary service FRU when CSB1 is removed
4871417 wfail fails wrong ports on certain DX ecc errors.
4875660 hpost -Q fails due to AXQ CASM discrepancy
4878056 wfail should consider some processor errors undiagnosable.
4890963 post needs to support lpost version 5.14.6
 
(from 114608-04)
 
4880549 hpost needs to support lbist for pciioc asic 2.5
4880811 Add wPCI 5015694-13 Rev 01, -13 Rev 50, and -12 Rev 50 to stage field_ict
 
(from 114608-03)
 
4822152 hwad optimizations or faster SC proc will break POST
4839477 post needs to support lpost version 5.14.5
4843254 JTAG TRST not asserted low on disconnected adapter
4851622 Processor frequency setting limited to 1250Mhz
4863496 Restrict use of MaxCPU board in split expander configuration
 
(from 114608-02)
 
4753686 Domain suffers Safari Bus error during device recognition in boot process
4803319 Problems with implementation of "allow_nonX150_rated_cpu_speed"
4814913 Need to accept new Ultrasparc III+ without a warning.
4815141 Need to accept Schizo 2.4 on wPCI without warnings.
4818581 POST Domain Advanced Test timeout exceeded on some domain configurations
4820554 hpost -H hang upon lock timeout
4823642 Remove up-level warnings for XMITS 2.0
4835023 Enable checking for DX pause timeout
4840328 wfail marks wrong port's memory when no trap expected.
4844692 Add WPCI 5015694-10 Rev. 51 to stage field_ict
 
(from 114608-01)
 
4807422 Need to adjust sram dimm timing for 900 Mhz procs

Patch Installation Instructions:
--------------------------------
For Solaris 8-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.
 
See Also:  System Management Services (SMS) 1.3 Installation Guide 
           Part No. 816-5320-10 
           Chapter 4, SMS 1.3 Additional Software Instructions
 
           Available at: http://www.sun.com/products-n-solutions/hardware/docs/Servers/High-End_Servers/Sun_Fire_15K/SW_FW_Documentation/SMS/index.html

Special Install Instructions:
-----------------------------
* To get the complete fix for 4974501, patch 114640-11, or higher, must be
  installed.
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).
 
 
Notes:
 
* When installing 114608-01 all domains must run at least a default
  level post for the fix to 4807422 to be applied.  The domains
  should undergo a setkeyswitch standby or off and then back to on.
 
* In order to get the complete fix for bugid 4839477 patch 115285-01 must be
  installed.
 
OTHELLO+ CP2140 (P/N 501-6754-01) INSTALLATION INSTRUCTIONS:
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
* To support installation of the Othello+ CP2140 controller (P/N 501-6754-01)
  onto the F12k/F15K System Controller (SC), this hpost patch (114608-07)
  must be installed along with the following required patches (if not already
  present):
 
	114609-02 (RFE 4817832, 4888914 = SSCPOST)
        115287-02 (RFE 4783744 = mand)
	115776-01 (RFE 4834834, BugId 4797191, 4942949 = SMS flashupdate)
	115954-01 (RFE 4783769 = SMS startup)
        115955-01 (RFE 4736411 = smsconfig)
        115957-01 (RFE 4817726, BugId 4896048 = SC OBP)
        116087-02 (RFE 4906317 = Solaris8 (point patch see:
                                        http://sunsolve.sun.com/point))
 
  Note that these additional patches are NOT required for the Nordica
  CP1500 (P/N 501-5994-06).  For Nordica CP1500, hpost patch 114608-07
  is "standalone" and forward- and backward-compatible, and therefore is
  "don't care" in regards to the patch numbers specified above

README -- Last modified date:  Friday, May 14, 2004

