Patch-ID# 117371-02
Keywords: sun fire 15k hpost redx libxcpost.so
Synopsis: SMS 1.4.1: hpost redx libxcpost.so patch
Date: May/28/2004


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.4.1

Xref: 

Topic: SMS 1.4.1:

Relevant Architectures: sparc

BugId's fixed with this patch: 4943893 4971389 4975645 5019759 5023600 5030572 5030612 5030965 5033832 5042013

Changes incorporated in this version: 4943893 4971389 4975645 5023600 5030572 5030612 5030965 5042013

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.4.1/bin/hpost
/opt/SUNWSMS/SMS1.4.1/bin/redx
/opt/SUNWSMS/SMS1.4.1/lib/libxcpost.so

Problem Description:

4943893 dstop during POST - AXQ and SDI are inconsistant
4971389 Jaguar SB indicated as primary service FRU during DR to a MCPU domain
4975645 Allow MaxCPU in split expander with AXQ 6.3
5023600 wfail should recognize EXBs reset during operation
5030572 Skip hsPCI+ workaround for AXQ 6.3
5030612 force_axq_xmits_throttle_vector doesn't work if only slot 0 present.
5030965 Accept AXQ 6.3 without warning
5042013 starcat post needs to support xmits 2.1 with out warning message
 
(from 117371-01)
 
5019759 Add retries for XIRs used for I/O test cage.
5033832 Add retries for XIRs during POST

Patch Installation Instructions:
--------------------------------
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).

README -- Last modified date:  Friday, May 28, 2004

