## Running a Diagnostic Test on a Device

To run a diagnostic test on a device:

1. Click Storage Automated Diagnostic Environment > Inventory.

The Devices page is displayed showing summary information for each system device.

2. Click the name of the device for which you want to run a diagnostic test.

Details for the selected device are displayed.

3. Click Diagnostics.

The Device Details page scrolls to a list of available diagnostic tests for the device.

4. Click to select the desired diagnostic test.

Note -

When running diagnostics on the Sun StorEdge 6130 Array, both controllers must be installed and online.

5. Click Run Test.

The Diagnostic Setup page is displayed for the selected diagnostic test.

6. Complete the diagnostic setup options and click Run.

The Test Results page is displayed and results are added when the test is completed.

Note -

Refer to the man pages for the CLI command diagnostic options for information about device diagnostics tests.

### Related Topics

- Reference: Sun StorEdge 6130 Array Diagnostics
- Viewing an Exception Report for System Devices
- Enabling/Disabling Fault Signature Analysis
- Recovering a Configuration