Patch-ID# 115951-01
Keywords: cp1500 sparc
Synopsis: Hardware/PROM: CP1500 OBP Firmware Update
Date: Aug/26/2003


Install Requirements: Additional instructions may be listed below                      
                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: Hardware/PROM

Unbundled Release: OBP 3.14.8

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4883296

Changes incorporated in this version: 4883296

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

CP1500.OBP.3.14.8
CP1500.OBP.3.14.8.Unix
CP1500.Release.Notes

Problem Description:

4883296 OBP 3.14.7 SCSI test fails "No selftest method"

Patch Installation Instructions:
-------------------------------- 
 
Refer to the special installation instructions described below.

Special Install Instructions:
----------------------------- 
 
 
    This patch has following files:
 
        CP1500.Release.Notes     - Firmware release notes
        CP1500.OBP.3.14.8.Unix   - OS level script for OBP update
        CP1500.OBP.3.14.8        - OBP firmware binary
 
 
    Firmware update sequence:
 
        1. Update OBP (OS level update method is highly
           recommended).
 
 
    Instructions for OS level SPARC firmware update script:
 
        o Copy "CP1500.OBP.3.14.8.Unix" file to the local
          disk of the CP1500 system.
 
        o Execute CP1500.OBP.3.14.8.Unix script as "root"
 
        o After flash update is done, halt OS to drop to
          OBP "ok" prompt. Power cycle the CP1500 board.
 
 
    Instructions for OBP level update:
 
        o Update the system flash using flash-update command
 
                ok flash-update <complete_path>/CP1500.OBP.3.14.8
 
        o Power cycle the CP1500 board.

README -- Last modified date:  Tuesday, August 26, 2003

