Patch-ID# 108983-02
Keywords: fcip ULP fibre channel panic tnf_mod_unload
Synopsis: SunOS 5.8: fcip patch
Date: 03/Apr/00

Solaris Release: 8

SunOS release: 5.8

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8: fcip patch

	NOTE:   Refer to Special Install Instructions section for 
                IMPORTANT specific information on this patch.

BugId's fixed with this patch: 4304890 4320876 

Changes incorporated in this version: 4320876

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/etc/name_to_major
/usr/include/sys/fibre-channel/ulp/fcip.h
/usr/lib/adb/fcip
/usr/lib/adb/fcip_dest
/usr/lib/adb/fcip_pkt
/usr/lib/adb/fcip_port_info
/usr/lib/adb/fcip_rt
/usr/lib/adb/fcipstr
/usr/lib/adb/la_els_farp
/usr/lib/adb/sparcv9/fcip
/usr/lib/adb/sparcv9/fcip_dest
/usr/lib/adb/sparcv9/fcip_pkt
/usr/lib/adb/sparcv9/fcip_port_info
/usr/lib/adb/sparcv9/fcip_rt
/usr/lib/adb/sparcv9/fcipstr
/usr/lib/adb/sparcv9/la_els_farp

Problem Description:

4320876 panic in fcip:_init when tnf_mod_unload() is called

(from 108983-01)

4304890 fcip: Integrate fcip ULP module

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

	NOTE:   To get the Sun FibreChannel Transport support for the 
                Qlogic PCI driver module and fcip driver modules, one
                needs to install the following new pkgs:

                SUNWfcip (Sun FCIP IP/ARP over FibreChannel Device Driver)
                SUNWfcipx(Sun FCIP IP/ARP over FibreChannel Device Driver 
                                (64 bit))
                SUNWqlc  (Qlogic ISP 2200/2202 Fibre Channel Device Driver)
                SUNWqlcx (Qlogic ISP 2200/2202 Fibre Channel Device Driver
                                (64 bit))

                The following patches need to be installed as well:

                108982-02 (or newer)    /kernel/misc/fctl and
                                        /kernel/misc/sparcv9/fctl patch
                108984-01 (or newer)    qlc adb macros patch
