Patch-ID# 108974-02
Keywords: atapi zip removable media sd uata LUN MMC
Synopsis: SunOS 5.8: sd and uata driver patch
Date: 20/Apr/00

Solaris Release: 8

SunOS release: 5.8

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8: sd and uata driver patch

	***********************************************************
	NOTE: This patch may contain one or more OEM-specific platform ports.
	      See the appropriate OEM_NOTES file within the patch for
	      information specific to these platforms.
 
	      DO NOT INSTALL this patch on an OEM system if a corresponding
	      OEM_NOTES file is not present (or is present, but instructs not
	      to install the patch), unless the OEM vendor directs otherwise.
	***********************************************************

	NOTE:	Refer to Special Install Instructions section for 
		IMPORTANT specific information on this patch.

BugId's fixed with this patch: 4285368 4285546 4305131 4313235 

Changes incorporated in this version: 4313235

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/kernel/drv/sd
/kernel/drv/sparcv9/sd
/kernel/drv/sparcv9/uata
/kernel/drv/uata

Problem Description:

4313235 sd: complains about attempt to read when no media present in a removable drive

(from 108974-01)

4285546 When atapi zip is read-write protected there are error
4285368 atapi zip with ufs can not be mounted on Ultra-10
4305131 sd: LUN not ready condition is not being handled properly

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

Reboot the system after patch installation.

	NOTE 1:	If you're using CDE 1.4, you MUST install the following
                patches:
 
                109165-01 (or newer)    CDE 1.4: dtfile patch 
                109167-01 (or newer)    CDE 1.4: Desktop Help Update Patch 
                108921-02 (or newer)    CDE 1.4: dtwm Patch 
 
		If you're using OpenWindows 3.8, you MUST install patch
                109463-01 (or newer).

        NOTE 2: To get the complete Removable Media functionality, one
		needs to install the following patches:

		108970-01 (or newer)	/usr/lib/fs/pcfs/fsck and
					/usr/lib/fs/pcfs/mkfs patch
		108972-01 (or newer)	/sbin/fdisk patch
		108977-01 (or newer)	libsmedia patch
		108968-01 (or newer)	vol/vold/rmmount patch
		108975-01 (or newer)    /usr/bin/rmformat and
					/usr/sbin/format patch
