Patch-ID# 109657-01
Keywords: panic isp DMA ddi_get_soft_state
Synopsis: SunOS 5.8: isp driver patch
Date: 24/May/00

Solaris Release: 8

SunOS release: 5.8

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8: isp driver patch

	***********************************************************
	NOTE: This patch may contain one or more OEM-specific platform ports.
	      See the appropriate OEM_NOTES file within the patch for
	      information specific to these platforms.
 
	      DO NOT INSTALL this patch on an OEM system if a corresponding
	      OEM_NOTES file is not present (or is present, but instructs not
	      to install the patch), unless the OEM vendor directs otherwise.
	***********************************************************

BugId's fixed with this patch: 4225880 4298594 4305985 4323441 

Changes incorporated in this version: 

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/kernel/drv/isp
/kernel/drv/sparcv9/isp

Problem Description:

4225880 panic in sd calling ddi_get_soft_state returning a Null pointer.
4298594 isp: driver does not resume after DR suspend
4305985 isp driver needs to work around PCI bus DMA problem
4323441 isp: multiinitiator differential cable failure causes node panic

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

Reboot the system after patch installation.
