Patch-ID# 108576-09
Keywords: Expert3D ifb ddx window
Synopsis: SunOS 5.8: Expert3D IFB Graphics Patch
Date: Oct/23/2000

Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: 

Unbundled Release:

Relevant Architectures: sun4u

BugId's fixed with this patch: 4287694 4288477 4288903 4292508 4294341 4294348 4297823 4299666 4304542 4309471 4303922 4299963 4306459 4307648 4311205 4310445 4306528 4307008 4304337 4314581 4275102 4312920 4325797 4281786 4320218 4281768 4330211 4332169 4312416 4334722 4336101 4331089 4327729 4330221 4329466 4338179 4338885 4339551 4342292 4339999 4345131 4343337 4345441 4345824 4318209 4308321 4346269 4343794 4319009 4351258 4350874 4354581 4349383 4371825 4374934 4362248 4368895 4373831 4367838 4370226 4342520 4361200 4366380 4374490 4375322 4381790

Changes incorporated in this version: 4381790

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

  /etc/init.d/ifbinit
  /etc/rc2.d/S91ifbinit
  /platform/sun4u/kernel/drv/ifb
  /platform/sun4u/kernel/drv/sparcv9/ifb
  /usr/lib/fbconfig/SUNWifb_config
  /usr/lib/ifb.ucode
  /usr/openwin/server/modules/ddxSUNWifb.so.1
  /usr/sbin/ifbdaemon

Problem Description: 

4381790 Patch 108576-08 causes error when installing MU3 on non-sun4u machines

(from 108576-08)
4366380 Ultra 80's with Expert3D graphics cards don't display properly
4374490 VSW502 testsuite in Xinerama gets sunifbPaintWindow PW_BORDER, border is tile er
4375322 0-length wide lines are not drawn
4371825 incorrect stereo modes listed for "fbconfig -res \?"
4374934 ifbconfig SEGVs when more than 32 video modes are available
4362248 Add 1152x900x120 stereo mode
4368895 issuing init 0 from CDE with high res. set (1920x1080 or 1920x1200) causes panic
4373831 1600x1200x75 video mode missing
4367838 power on default clock is wrong
4370226 fbconfig should display monitor information
4342520 Expert3D: pointer leaves on choosing command line login from dtlogin
4361200 running an opengl demo on xinerama on 2 IFB's on Excalibur causes Xsun hang

(from 108576-06)
4349383 Acroread doesn't redraw properly on IFB lite after dragging text around

(from 108576-05)
4350874 screen corrupted and unusable after framebuffer pm
4351258 CPR fails when board as been power managed
4354581 DMA buffers can leak

(from 108576-04)
4318209 fbconfig should give more hardware information
4308321 SUNWifb_config -prconf no data for  monitor sense,  or slave
4346269 Drop framebuffer pm from SU2
4319009 Add display list functions to IFB driver

(from 108576-03)
4332169 ifbdaemon needs to allow for more than one version of the geometry engine
4330211 SUNWifb_config should print out the frame buffer type
4327729 Need another variant of ifb_open()
4312416 Expert3D driver needs Solaris 8 power management functions
4330221 available resolutions should depend on the available FB memory
4334722 IFB driver should fail to attach in selected 66MHz slots
4336101 Solid fill rate is too low
4329466 IFB multiview feature identificaton incorrect
4331089 Need kernel support for multiple revisions
4338179 Expert3D prom incorrectly sets tomcat configuration register
4338885 108576-03 causes a panic while performing E* tests on IFB
4339551 IFB Direct Burst memory PLL tune value is not optimal
4342292 ifb pci timeouts on PM resume
4339999 Double buffering problem with multiple views in Unigraphics
4345131 video timings not at advertised rates                                   
4343337 graphical installation hangs on unsupported OS versions
4343794 Expert3D: fbconfig -defaults cause the screen gets black out.
4345441 v_freq property set incorrectly for 1152x900x76
4345824 kernel panics when booted in 32 bit mode

(from 108576-02)
4306459 SUNWifb_config causes fbconfig -dev /dev/fbs/ifb1 -help to fail
4304542 FTC copyimage2 hang
4320218 regressions in Xtest testing
4312920 graphics tests running on IFB are causing the Xserver and window manager to exit
4325797 Can't start CDE using PGX32 and ifb in a particular sequence
4303922 Xserver crashes with 24-bit server,  Non-Linear Normal Visual as default
4310445 Expert3D ddx does not advertise shared memory functions
4307648 add stereo support on Expert3d for 24" t-rex monitor
4309471 Expert3D forces composite sync for all video modes
4281768 Window system dies if you run an XGL program on IFB.
4281786 Polling fails, eventually ceases, and no alarms or anything happen
4306528 SUNWifb_config cannot set defoverlay on windows level, propts okay
4307008 Add 1280x768x56 video mode for PDP-502MX
4311205 Add QXGA resolution support to Expert3D
4299963 fbconfig without arguments defaults to /dev/fbs/ifb0 when /dev/fb -> fbs/ifb1
4314581 -defoverlay true does not work properly
4304337 Stray lines left in main window after moving graphics window in Unigraphics
4275102 Previously popped up menus effect later selection in Unigraphics

(from 108576-01)
4299666 stereo 3D display shows incorrect images
4294348 GLX pixmap fails
4288903 bad application causes X server crash
4294341 higher resolution double buffered animation shows intermittent flashing
4297823 linear visuals aren't gamma corrected if no gamma value is given in OWconfig
4288477 scrambled context causes hang
4292508 ProE 8-bit startup window leaves damage on 24-bit graphics canvas
4287694 Moving a stereo window does not copy the right buffer

Patch Installation Instructions: 
-------------------------------- 

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
	example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
	example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 
	After patch installation, reboot the system to load the newly
	installed driver.
