Patch-ID# 112429-08
Keywords: SANbox Manager fiber channel administration
Synopsis: Sun StorEdge Network Fiber Channel 4.0: SANbox Manager Patch
Date: Jan/10/2003

GUI Version: 1.03.46

Install Requirements: None                      
                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: StorEdge Network Fiber Channel

Unbundled Release: 4.0

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4672499 4679369 4681562 4685666 4688041 4691392 4704180 4706259 4716947 4719377 4738520 4796944

Changes incorporated in this version: 4796944

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/usr/opt/SUNWsmgr2/bin/SANsurfer2.jar
/usr/opt/SUNWsmgr2/firmware/SANbox1/08040233.fls
/usr/opt/SUNWsmgr2/firmware/SANbox1/16040233.fls
/usr/opt/SUNWsmgr2/firmware/SANbox2/fullimage.1.3.60.00

Problem Description:

4796944 2G 8-port switch becomes unreachable (using firmware 1.3.60)
 
(from 112429-07)
(from 112429-06)
4738520 2G 8-port switch becomes unreachable until power cycle
 
(from 112429-05)
(from 112429-04)
(from 112429-03)
(from 112429-02)
4672499 Restore fabric takes too long when invoked - Refresh topology.
4681562 Firmware upload did not complete, status unknown!
4691392 qLogic 2 GigaBit 16 Port Switch shows 2 GigaByte throughput (i.e., 2G)!
4704180 Admin mode CLI executed in regular user.
4706259 Switch reset cause login timeout.
4716947 2g switch with finisar SFP will not work with loopback cable
4719377 storade cannot draw topology correctly with 2G qlogic switch
No Bug# Port 0 problem - After ISL cable pull, GA_NXT rejected when port 0 is F_Port and leadville driver requests port_address - 1.
 
(from 112429-01)
4679369 T3B: Removing one slice causes ALL LUNs on T3B to become unusable when using an
4685666 switch network netmask inconsistent depending on switch's bootmethod
4688041 Switch reset causes to go switch ISL offline resulting IOs failure.

Patch Installation Instructions:
-------------------------------- 
For Solaris 8 releases, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
None.

README -- Last modified date:  Friday, January 10, 2003

