## Event and Severity Map Page

This page displays the events the agents are monitoring and the corresponding severity levels for each.

Field | Description
--- | ---
Device | Lists the device type; for example, Sun 3310 or a Sun StorEdge 6020 array.
Attribute Name | The event name (for example, `disk_status` or `alarmEvent`).
Value | The attribute value that correlates to the attribute name. It is possible to have multiple values for an attribute name (for example, for `disk_status` (attribute name), the values might be bad drive, offline, and online).
Severity | Indicates the severity of the alarm that corresponds to that device. for example, Information Major Critical Down
Action required | Whether the event requires service action (red events, which indicate the system has an error or the system is down) or does not require service (white events, which indicate information only, or yellow events, which indicate a warning).

### Related Topics

- Displaying an Event and Severity Mapping Report
- Using Event and Severity Mapping