## Overview

Sun StorEdge Solutions products, including the Sun StorEdge 6920 system, are logical storage devices created from Sun switches, Sun StorEdge storage arrays, Sun virtualization engines (for the Sun StorEdge 3900 and 6900 system) and a Storage Service Processor.

These components are preconfigured into a single product that includes a version of the Storage Automated Diagnostic Environment software on the Storage Service Processor (the Storage Automated Diagnostic Environment System Edition). The version of the Storage Automated Diagnostic Environment in the solution rack can be accessed like any other the Storage Automated Diagnostic Environment master agent with a browser pointing to the IP address of the Storage Service Processor.

The primary functions of the Storage Automated Diagnostic Environment application, which comprises the diagnostic and monitoring software, are:

- Device health monitoring
- Event generation
- Topology discovery and presentation
- Diagnostics
- Revision maintenance
- Device and field-replaceable unit (FRU) reporting

### Related Topics

- Enabling Notification
- Configuring System-Wide Settings
- Monitoring Events and Devices
- Servicing Tasks
- Reviewing Logs and Core Files
- Using Reports