## System Timeouts Page

This page enables you to specify the timeout values used for various system functions.

Field | Description
Ping | The timeout used to perform a ping. The default is 10 seconds.
Email | The timeout used when sending email messages. The default is 30 seconds.
Sun Storage Arrays (http tokens) | The timeout used when extracting token information from an array. The default is 60 seconds.
SNMP access | The timeout used to query switches that support Simple Network Management Protocol (SNMP). The default is 60 seconds.
Discman (Discovery) | The Discman discovery timeout. The default is 1200 seconds.
Power Sequencer | The amount of time before a lack of acknowledgement from the power sequencer is determined to be a fault.
Submit | Click to enable specified timeout values.
Defaults | Click to return timeouts to their default values.

### Related Topics

- Setting System Timeouts
- Testing an Email Address
- Setting Up the SNMP Trap Notification Provider