## Entering and Erasing MAC Addresses

To enter a MAC address:

1. Go to the Sun Web Console and click Storage Automated Diagnostic Environment.
2. Click Service > Sun Solution Series > Ethers.
3. Type a MAC address for each IP address, and click Update Ethers to update the `/etc/ethers` file.

Note -

MAC addresses for each device are found on a sticker attached to the back panel of the device.

4. Clcik Update Ethers.
5. Turn power off and on for each device for which you have assigned a MAC address.

To erase a MAC address:

1. Go to the Sun Web Console and click Storage Automated Diagnostic Environment.
2. Click Service > Sun Solution Series > Ethers.
3. Erase the MAC address, and click Update Ethers to delete the entry from the `/etc/ethers` file.

### Related Topics

- Using MAC Addresses