## Mapping an Initiator to Volumes

To map initiators to a volume:

1. Go to the Sun Web Console page and click SE6920 Configuration Service.
2. Click Storage > Physical > Initiators.
3. Click the initiator that you want to map.

The Initiator Details page is displayed and the Map button is enabled.

4. Click Map.

The Map Initiator wizard is displayed.

5. Select the volumes to which you want to map the initiator. Additionally, select the LUN (0 to 255), and the Permissions (Read/Write, Read Only). Click Next.
6. Review the specified information. If you are satisfied, click Finish. Otherwise, click Previous to make changes.

### Related Topics

- Managing Initiators
- Creating an Initiator
- Configuring Storage Volumes