## Performing a Partial Shutdown

When you perform a partial shutdown, the system is in the following state:

- The Storage Service Processor in the base cabinet remains powered on.
- The Storage Service Processor Accessory tray remains powered on.
- All storage arrays are powered off.
- The Data Services Platform is powered off.
- Only the Power Available LED on the power sequencers are lit.

To turn the system's power off:

1. Go to the Sun Web Console page and click SE6920 Configuration Service.
2. Click Administration > General Settings.
3. Click the System Partial Shutdown button.
4. Click OK to confirm you want to perform a partial shutdown.

The following message is displayed on the General Settings page:

Partial system shutdown completed successfully

To restore the system, use the following procedure:

1. Go to the Sun Web Console page and click SE6920 Configuration Service.
2. Click Administration > General Settings.
3. Click the Restart button.

The power sequencers in the base cabinet and any expansion cabinets are activated and they restore power to the components.

### Related Topics

- About Lights-Out Management