## Device Page

This page displays a list of system devices and allows you to display various types of information for each.

Field | Description
Host | The name of the host; for example, host.domain.sun.com.
Type | The device type; for example, array or dsp.
Device | The name of the device; for example, host.domain.sun.com-array01.
Alarms | The severity of the alarm. Alarm severities include: Black - Down Red - Critical Yellow - Major Blue - Information Click the severity icon for an alarm to access options for obtaining more information about the alarm and the device associated with it. The options are as follows: Summary Report - Describes the selected device in detail. Alarms - Displays a summary of alarms or the device. Event Log - Displays all events generated against the selected device. Detailed Event Log - Displays, in nested detail, all monitored attributes for the selected device. Alarms & Graph - Displays a sub-topology of the selected device and its immediate neighbors. Diagnostics - Enables you to start a diagnostic test on the device.
Last Probe | The date and time the device was probed and events were generated; for example, 11-04 11:37:20.

The Device Page allows you to display the following information for listed devices:

- 6920 Device Summary Report
- Array Device Summary Report
- DSP Device Summary Report
- SP Device Summary Report
- Device Alarms Summary
- Device Event Log Summary
- Device Alarms & Graph Summary
- Device Diagnostics Page

### 6920 Device Summary Report

The following table identifies the content of a device summary report for the Sun StorEdge 6920.

Field | Description
System
Name | The assigned name for the Sun StorEdge 6920.
Model | The model designation of the Sun StorEdge 6920.
Revision | The firmware revision level of the diagnostic and monitoring software.
Power Sequencer | Not applicable at this time.
System Components
Component | The type of the system component.
Name | The name of the system component.
Status | The current status of the system component.
Ports
Port | The number of the port.
Id | A number that identifies the system location of the port.
WWN | The world wide name (WWN) of the port.
Status | The current status of the port.
Comm: | The communication status of the port.
FRUs
FRU | An identification number for the FRU.
Type | The system component in which the FRU resides.
Name | The name of the FRU.
Rev) | The current revision level of the FRU.
Status | The current status of the FRU.
Volumes
# | The volume number.
Name | The assigned name of the volume.
Capacity | The storage capacity of the volume.
Id | A identification number for the volume.

### Related Topics

- Monitoring Devices Using the Device Summary Report
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report

### Array Device Summary Report

The following table identifies the content of a device summary report for the Sun StorEdge 6020 array.

Field | Description
Array
Name | The device name and the device IP address.
WWN | The worldwide name (WWN) of the array controllers.
Agent | The name of the host that is monitoring the array.
Comm: | The communication status of the array.
Type | The array type and array configuration; for example, a 6020 array can be configured in a 2x2, 2x4, or a 2x6 configuration.
Revision | The firmware revision level of the array.
mp_support | Indicates if the array supports multi-path operation.
disk_scrubber | Indicates if the array is configured for continuous volume verification.
Array Components
Type | The type of array component.
Identification | The brand designation of the device component. For example, for a 6020 array disk, the identification for the component might be SEAGATE/<serial number>.
Location | The correct position for the array component in a Sun StorEdge Solution rack; for example, u1d1.
Status | The status of the array component; for example, ready-enabled, online, or not installed.
Rev./Info | Revision information for the array component.

### Related Topics

- Monitoring Devices Using the Device Summary Report
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report

### DSP Device Summary Report

The following table identifies the content of a device summary report for the Sun Data Services Platform.

Field | Description
DSP
Name | The assigned DSP device name.
IP | The IP address of the DSP.
Power | The status of front-end (A) and back-end power (B).
Volumes | The number of volumes recognized by the DSP..
Revision | The firmware revision level of the DSP.
RevDate | The date of the last revision update.
Fan | The status of the DSP fan.
Ports | The number of ports supported by the DSP.
Virtual Disks | The number of created virtual disks.
Cards | The number of cards currently installed in the DSP.
FRUs
Location | The position of the FRU component in the DSP.
Type | The type of DSP FRU component.
Class | A description of the FRU type.
Model/Serial | The model number and serial number of the DSP component.
HW/PCB | The hardware and printed circuit board revision.
#Cpus/Ports | The number of CPUs and Ports on the DSP card.
Status | The status of the DSP component; for example, Booting/Standing By, Ready/Normal, On, or Failed-Absent.
Temp | The last measured temperature of the DSP component.
Ports
Port# | The system identification number of the port.
Slot/Port | The card slot and port location of the DSP port.
Type | The type of DSP port, including the port speed and connection type. For example, 2GBIC-nport-fabric, SCSI, where 2GBIC indicates a 2 Gigabyte port and nport-fabric indicates a fibre channel port.
State | Indicates whether the DSP port is online of offline.
WWN/Remote WWN | The worldwide name (WWN) of the port and the WWN of the attached remote port.
Virtual Disks (Array Slices)
Product | Storage array type.
WWN | The worldwide name (WWN) of the virtual disk.
Revision | The current revision level of the virtual disk.
RawSize | The physical size of the virtual disk.
FC-Servers
Name | The name of the FC-server assigned by the DSP.
WWN | The world wide name (WWN) of the FC-server.
Status | The current status of the FC-server.
SVSD | The host initiator.
Mapped LUNs
Element | The DSP volume to which the LUN is mapped.
State | The current state of the LUN.
Type | The type of LUN.
Condition | The current condition of the LUN.
Capacity | The capacity of the LUN.
WWN | The world wide name (WWN) of the LUN.

### Related Topics

- Monitoring Devices Using the Device Summary Report
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report

### SP Device Summary Report

The following table identifies the content of a device summary report for the Sun Storage Service Processor.

Field | Description
Filesystem | The name of a SP filesystem.
Mounted | The mounting point for the SP filesystems.
Capacity | The capacity of the SP file system.
Ap_Id | A list of Universal Serial Bus (USB) appliances used by the filesystem.
Receptacle | Whether the USB is connected or empty.
Condition | USB device status.
SUNWstads Patches | Installed system patches that have been installed for the SP.

### Related Topics

- Monitoring Devices Using the Device Summary Report
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report

### Device Alarms Summary

This summary displays current alarms for a selected device and allows you to access more detailed information about the alarms and the associated device.

Field | Description
Page | List of available information for the subject device.
Severity (icon) | The severity rating of the alarm. Event severities include: Black - Down Red - Critical Yellow - Major Blue - Information
Alarm Details | Click to display more detailed information about the corresponding alarm.
Show Sub-Events | Click to display all sub-events associated with the displayed events.
Hide Sub-Events | Click to hide all sub-events associated with the displayed events.
Delete All Alarms | Click to delete all alarms for the selected device.

### Related Topics

- Monitoring Device Alarms
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Devices Using the Device Summary Report
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report

### Device Event Log Summary

This page displays the event log for a selected device.

Field | Description
Page | List of available information for the subject device.
Time | The date and time of the event.
Host | The name of the device in which the device component resides.
Severity | The severity rating of the alarm. Event severities include: Black - Down Red - Critical Yellow - Major Blue - Information
Event | The name of the event.
Description | Information about the event.

### Related Topics

- Displaying the Event Log for a Specific Device
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Devices Using the Device Summary Report
- Monitoring Device Alarms
- Monitoring Devices Using the Alarms & Graph Report

### Device Alarms & Graph Summary

This page displays a graphical view of the storage devices and allows you to click on a device to view alarms associated with the device.

Field | Description
Connection Details | A graphical illustration with all major FRUs labeled.
Alarm Details | Click to display Event Advisor.

### Related Topics

- Monitoring Devices Using the Alarms & Graph Report
- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Devices Using the Device Summary Report
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device

### Device Diagnostics Page

This page displays a list of tests that are available for a selected device and allows you to click on a test name to initiate that test. For more information on diagnostics, see About Diagnostic Tests.

### Related Topics

- About Monitoring Devices
- Starting and Stopping Monitoring on a Device
- Starting and Stopping Monitoring Agents
- Monitoring Devices Using the Device Summary Report
- Monitoring Device Alarms
- Displaying the Event Log for a Specific Device
- Monitoring Devices Using the Alarms & Graph Report