## Starting and Stopping Continuous Volume Verify for a Specific Array

To enable Continuous Volume Verify to run on an array:

1. Go to the Sun Web Console and click Storage Automated Diagnostic Environment.
2. Click Administration > General Maintenance > Maintain Devices.
3. Click the name of the array on which you want Continuous Volume Verify to run.

Information and options for the array are displayed.

4. From the "Run `vol verify' continuously" list, select On.
5. Click Update.

Continuous Volume Verify will run on the array according to options defined in the Continuous Volume Verify page. See Scheduling Continuous Volume Verify for more information.

To disable Continuous Volume Verify for an array:

6. Go to the Sun Web Console and click Storage Automated Diagnostic Environment.
7. Click Administration > General Maintenance > Maintain Devices.
8. Click the name of the array on which you want to stop Continuous Volume Verify.

Information and options for the array are displayed.

9. From the "Run `vol verify' continuously" list, select Off.
10. Click Update.

### Related Topics

- Using Continuous Volume Verify
- Scheduling Continuous Volume Verify
- Stopping Continuous Volume Verify for All Devices
- Displaying Continuous Volume Verify Results